{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":11,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M"]
[]
[]
[]
[]
["","","","","","2AMXM40M2V1B","2AMXM40M3V1B","2AMXM40M4V1B","2AMXM50M2V1B","2AMXM50M3V1B","2AMXM50M4V1B"]
["المروحة","معدل تدفق الهواء","التبريد","منخفض جداً","m³/min","30","","","34"]
["","","التدفئة","منخفض جداً","m³/min","32","","","34"]
["مستوى طاقة الصوت","التدفئة","","","dBA","","","62","","","62"]
["","التبريد","","","dBA","","","60","","","60"]
["المروحة","معدل تدفق الهواء","التبريد","منخفض جداً","cfm","1059","","","1200"]
["","","التدفئة","منخفض جداً","cfm","1130","","","1200"]
["الأبعاد","الوحدة","","الارتفاع","mm","550","550","550","550","550","550"]
["","","","العرض","mm","765","765","765","765","765","765"]
["","","","العمق","mm","285","285","285","285","285","285"]
["الوزن","الوحدة","","","kg","36","36","36","41","41","41"]
["محرك المروحة","السرعة","التبريد","منخفض جداً","rpm","760","500","500","890","500","500"]
["","","التدفئة","منخفض جداً","rpm","820","320","320","890","500","500"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-10","","46.0","-10","","46.0"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","46","","-10","46","","-10"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-15","","-15","-15","","-15.0"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","18","","18.0","18","","18.0"]
["Sound pressure level","Cooling","","High","dBA","","46","46","","48","48"]
["","","","Nom.","dBA","48","","","46"]
["","Heating","","High","dBA","","48","48","","50","50"]
["","","","Nom.","dBA","50","","","48"]
["سائل تبريد","النوع","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","السعة","","","kg","0.88","0.88","0.88","1.15","1.15","1.15"]
["","السعة","","","tCO2Eq","0.6","0.59","0.6","0.8","0.78","0.78"]
["","GWP","","","","675","675.0","675","675","675","675"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","20","20 (1)","20 (1)","20","20 (1)","20 (1)"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)"]
["","Level difference","IU - OU","Max.","م","15","15.0","15","15","15.0","15"]
["","","IU - IU","Max.","م","7.5","7.5","7.5","7.5","7.5","7.5"]
["وصلات الأنابيب","طول الأنابيب الإجمالي","النظام","فعلي","م","30","30","30","30","30","30"]
["Standard Accessories","دليل التركيب","","","","دليل التركيب","1","1","1","1","1"]
["","سدادة المصرف","","","","سدادة المصرف","1","1","1","1","1"]
["","حقيبة المسامير اللولبية","","","","حقيبة المسامير اللولبية","1","1","1","1","1"]
["نطاق كفاءة استخدام الطاقة","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-230-240","220-230-240","220-240","220-230-240","220-230-240"]
["Notes","","","","","(1) - يحتوي على غازات الاحتباس الحراري المفلورة","","","(1) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["","","","","","","(1) - لغرفة واحدة","(1) - لغرفة واحدة","","(1) - لغرفة واحدة","(1) - لغرفة واحدة"]
["","","","","","","(2) - انظر الرسم المنفصل لنطاق التشغيل","(2) - انظر الرسم المنفصل لنطاق التشغيل","","(2) - انظر الرسم المنفصل لنطاق التشغيل","(2) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","","(3) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(3) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","","(3) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(3) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","","","(4) - يحتوي على غازات الاحتباس الحراري المفلورة","(4) - يحتوي على غازات الاحتباس الحراري المفلورة","","(4) - يحتوي على غازات الاحتباس الحراري المفلورة","(4) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["Standard Accessories","مجموعة المخفض","","","","","","","1","1","1"]