{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXF-B"]
[]
[]
[]
[]
["","","","","","3AMXF52B2V1B"]
["الأبعاد","الوحدة","","الارتفاع","mm","734"]
["","","","العرض","mm","974"]
["","","","العمق","mm","401"]
["الوزن","الوحدة","","","kg","57.0"]
["محرك المروحة","السرعة","التبريد","منخفض جداً","rpm","420"]
["","","التدفئة","منخفض جداً","rpm","420"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","46"]
["Sound pressure level","Cooling","","Nom.","dBA","46.0"]
["","Heating","","Nom.","dBA","47.0"]
["سائل تبريد","النوع","","","","R-32"]
["","السعة","","","kg","1.65"]
["","السعة","","","tCO2Eq","1.11"]
["","GWP","","","","675"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","25 (1)"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 30m)"]
["","Level difference","IU - OU","Max.","م","15.0"]
["","","IU - IU","Max.","م","7.5"]
["وصلات الأنابيب","طول الأنابيب الإجمالي","النظام","فعلي","م","50"]
["Standard Accessories","دليل التركيب","","","","1"]
["","غطاء المصرف","","","","3"]
["","سدادة المصرف","","","","1"]
["","مجموعة المخفض","","","","1"]
["","حقيبة المسامير اللولبية","","","","1"]
["نطاق كفاءة استخدام الطاقة","","","","","A+++ ~ D"]
["Notes","","","","","(1) - لغرفة واحدة"]
["","","","","","(2) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","(3) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","","(4) - يحتوي على غازات الاحتباس الحراري المفلورة"]