{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-M"]
[]
[]
[]
[]
["","","","","","3AMXM52M3V1B","3AMXM52M2V1B"]
["Sound pressure level","Heating","","Nom.","dBA","47"]
["","Cooling","","Nom.","dBA","46"]
["Standard Accessories","دليل التركيب","","","","1"]
["","حقيبة المسامير اللولبية","","","","1"]
["","سدادة المصرف","","","","1"]
["","سدادة التصريف (1)","","","","6"]
["","سدادة التصريف (2)","","","","3"]
["","انزع ملصق الغاز F","","","","1"]
["","ملصق سائل التبريد الإضافي","","","","1"]
["Refrigerant","Charge","","","TCO2Eq","1.2"]
["","GWP","","","","675"]
["","Charge","","","kg","1.8"]
["","النوع","","","","R-32"]
["Fan motor","Speed","Cooling","منخفض جداً","rpm","420"]
["","","Heating","منخفض جداً","rpm","420"]
["Piping connections","Level difference","IU - IU","Max.","م","7.5"]
["","","IU - OU","Max.","م","15"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 30m)"]
["","طول الأنابيب الإجمالي","النظام","فعلي","م","50"]
["Compressor","Type","","","","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","mm","868"]
["","","","العمق","mm","320"]
["","","","الارتفاع","mm","734"]
["الوزن","الوحدة","","","kg","57"]
["Power supply","الطور","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["","","","","","(2) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","(3) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["المروحة","معدل تدفق الهواء","التبريد","منخفض جداً","m³/min","","24"]
["","","التدفئة","منخفض جداً","m³/min","","24"]
["","","","منخفض جداً","cfm","","847"]
["","","التدفئة","منخفض جداً","cfm","","847"]
["الأبعاد","الوحدة","","الارتفاع","mm","","734"]
["","","","العرض","mm","","868"]
["","","","العمق","mm","","320"]
["الوزن","الوحدة","","","kg","","57"]
["محرك المروحة","السرعة","التبريد","منخفض جداً","rpm","","420"]
["","","التدفئة","منخفض جداً","rpm","","420"]
["Compressor","Type","","","","","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","","-15"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","","18"]
["Sound pressure level","Cooling","","Nom.","dBA","","46"]
["","Heating","","Nom.","dBA","","47"]
["سائل تبريد","النوع","","","","","R-32"]
["","السعة","","","kg","","1.80"]
["","السعة","","","tCO2Eq","","1.2"]
["","GWP","","","","","675"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","","25"]
["Piping connections","Additional refrigerant charge","","","kg/m","","0.02 (for piping length exceeding 30m)"]
["","Level difference","IU - OU","Max.","م","","15"]
["","","IU - IU","Max.","م","","7.5"]
["وصلات الأنابيب","طول الأنابيب الإجمالي","النظام","فعلي","م","","50"]
["Standard Accessories","Installation manual","","","","","1"]
["","Drain plug","","","","","1"]
["","Screw bag","","","","","1"]
["وحدة التزويد بالطاقة","الطور","","","","","1~"]
["Power supply","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]