{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-M"]
[]
[]
[]
[]
["","","","","","3MXM40M2V1B","3MXM52M2V1B","3MXM68M2V1B"]
["المروحة","معدل تدفق الهواء","التبريد","منخفض جداً","m³/min","24","24","24.1"]
["","","التدفئة","منخفض جداً","m³/min","24","24","24.1"]
["","","","منخفض جداً","cfm","847","847","851"]
["","","التدفئة","منخفض جداً","cfm","847","847","851"]
["الأبعاد","الوحدة","","الارتفاع","mm","734","734","734"]
["","","","العرض","mm","868","868","868"]
["","","","العمق","mm","320","320","320"]
["الوزن","الوحدة","","","kg","57","57","62"]
["محرك المروحة","السرعة","التبريد","منخفض جداً","rpm","420","420"]
["","","التدفئة","منخفض جداً","rpm","420","420"]
["Compressor","Type","","","","ضاغط متأرجح محكم مانع للتسريب","","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-10","-10","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","46","46","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-15","-15","-15"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","18","18","18"]
["Sound pressure level","Cooling","","Nom.","dBA","46","46","48"]
["","Heating","","Nom.","dBA","47","47","48"]
["سائل تبريد","النوع","","","","R-32","R-32","R-32"]
["","السعة","","","kg","1.80","1.80","2.0"]
["","السعة","","","tCO2Eq","1.2","1.2","1.4"]
["","GWP","","","","675","675","675"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","25","25","25"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 30m)","0.02 (for piping length exceeding 30m)"]
["","Level difference","IU - OU","Max.","م","15","15","15"]
["","","IU - IU","Max.","م","7.5","7.5","7.5"]
["وصلات الأنابيب","طول الأنابيب الإجمالي","النظام","فعلي","م","50","50"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["ضاغط","نوع","","","","","ضاغط متأرجح محكم مانع للتسريب"]
["Standard Accessories","Drain cap","","","","","","9"]
["","Reducer assembly","","","","","","1"]