{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":8,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXS-K"]
[]
[]
[]
[]
["","","","","","3MXS40K3V1B","3MXS40K3V1B2","3MXS40K2V1B"]
["Sound pressure level","Heating","","Nom.","dBA","47","47"]
["","Cooling","","Nom.","dBA","46","46"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","سدادة المصرف","","","","1","1"]
["Refrigerant","Charge","","","TCO2Eq","4.2","4.2"]
["","GWP","","","","2,087.5","2,087.5"]
["","Charge","","","kg","2.0","2.0"]
["","النوع","","","","R-410A","R-410A"]
["Piping connections","Level difference","IU - IU","Max.","م","7.5","7.5"]
["","","IU - OU","Max.","م","15","15"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 30m)","0.02 (for piping length exceeding 30m)"]
["","طول الأنابيب الإجمالي","النظام","فعلي","م","50","50"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","mm","936","936"]
["","","","العمق","mm","300","300"]
["","","","الارتفاع","mm","735","735"]
["الوزن","الوحدة","","","kg","49","49"]
["Power supply","الطور","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","230","230"]
["Notes","","","","","(1) - يحتوي على غازات الاحتباس الحراري المفلورة","(1) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["الأبعاد","الوحدة","","الارتفاع","mm","","","735"]
["","","","العرض","mm","","","936"]
["","","","العمق","mm","","","300"]
["الوزن","الوحدة","","","kg","","","49"]
["Compressor","Type","","","","","","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","","","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","","","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","","","-15"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","","","15.5"]
["Sound pressure level","Cooling","","Nom.","dBA","","","46"]
["","Heating","","Nom.","dBA","","","47"]
["سائل تبريد","النوع","","","","","","R-410A"]
["","السعة","","","kg","","","2.0"]
["","السعة","","","tCO2Eq","","","4.2"]
["","GWP","","","","","","2087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","","","50"]
["Piping connections","Additional refrigerant charge","","","kg/m","","","0.02 (for piping length exceeding 30m)"]
["","Level difference","IU - OU","Max.","م","","","15"]
["","","IU - IU","Max.","م","","","7.5"]
["Standard Accessories","Drain plug","","","","","","1"]
["وحدة التزويد بالطاقة","الطور","","","","","","1~"]
["Power supply","Frequency","","","Hz","","","50"]
["","Voltage","","","V","","","230"]