{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXM-M"]
[]
[]
[]
[]
["","","","","","4MXM68M2V1B","4MXM80M2V1B"]
["Sound pressure level","Heating","","Nom.","dBA","49","49"]
["","Cooling","","Nom.","dBA","48","48"]
["Standard Accessories","دليل التركيب","","","","1","1"]
["","حقيبة المسامير اللولبية","","","","1","1"]
["","سدادة المصرف","","","","1","1"]
["","غطاء المصرف","","","","9","9"]
["","مجموعة المخفض","","","","1","1"]
["Refrigerant","Charge","","","TCO2Eq","1.4","1.6"]
["","GWP","","","","675","675"]
["","Charge","","","kg","2.00","2.4"]
["","النوع","","","","R-32","R-32"]
["Piping connections","Level difference","IU - IU","Max.","م","7.5","7.5"]
["","","IU - OU","Max.","م","15","15"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 30m)","0.02 (for piping length exceeding 30m)"]
["","طول الأنابيب الإجمالي","النظام","فعلي","م","60","70"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","mm","320","320"]
["","","","العمق","mm","868","868"]
["","","","الارتفاع","mm","734","734"]
["الوزن","الوحدة","","","kg","63","67"]
["Fan","Air flow rate","Heating","منخفض جداً","cfm","851.0","851.0"]
["","","Cooling","منخفض جداً","cfm","851","851.0"]
["Power supply","الطور","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - يحتوي على غازات الاحتباس الحراري المفلورة","(1) - يحتوي على غازات الاحتباس الحراري المفلورة"]