{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5XXM-A"]
[]
[]
[]
[]
["","","","","","5XXM68A2V1B","5XXM90A2V1B"]
["الأبعاد","الوحدة","","الارتفاع","mm","734","734"]
["","","","العرض","mm","1040","1040"]
["","","","العمق","mm","408","408"]
["الوزن","الوحدة","","","kg","69.0","73.0"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-10","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","50","50"]
["Sound pressure level","Cooling","","Nom.","dBA","48.0 (2)","52.0 (2)"]
["","Heating","","Nom.","dBA","49.0 (2), 51.0 (3)","53.0 (2), 55.0 (3)"]
["سائل تبريد","النوع","","","","R-32","R-32"]
["","السعة","","","kg","2.00","2.40"]
["","السعة","","","tCO2Eq","1.35","1.62"]
["","GWP","","","","675","675.0"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","25 (4) (5)","25 (5) (4)"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 30m) (2)","0.02 (for piping length exceeding 30m)"]
["","Level difference","IU - OU","Max.","م","15.0 (5)","15.0 (5)"]
["","","IU - IU","Max.","م","7.5 (5)","7.5 (5)"]
["وصلات الأنابيب","طول الأنابيب الإجمالي","النظام","فعلي","م","60","75"]
["Standard Accessories","دليل التركيب","","","","1","1"]
["","غطاء المصرف","","","","3","3"]
["","سدادة المصرف","","","","1","1"]
["","مجموعة المخفض","","","","1","1"]
["","حقيبة المسامير اللولبية","","","","2","2"]
["نطاق كفاءة استخدام الطاقة","","","","","A+++ ~ D","A+++ ~ D"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~"]
["Power supply","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - انظر الرسومات المنفصل للحصول على نطاق التشغيل","(1) - انظر الرسومات المنفصل للحصول على نطاق التشغيل"]
["","","","","","(2) - For DX combination","(2) - For DX combination"]
["","","","","","(3) - For Space heating operation of CHVX07 unit","(3) - For Space heating operation of CHVX07 unit"]
["","","","","","(4) - لغرفة واحدة","(4) - لغرفة واحدة"]
["","","","","","(5) - For combination with FBA71/100/125 refer to installation manual","(5) - For combination with FBA71/100/125 refer to installation manual"]
["","","","","","(6) - يحتوي على غازات الاحتباس الحراري المفلورة","(6) - يحتوي على غازات الاحتباس الحراري المفلورة"]