{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-A"]
[]
[]
[]
[]
["","","","","ABQ71AV1","ABQ100AV1","ABQ125AV1","ABQ140AV1"]
["Fan","External static pressure","Super high","باسكال","78","118","147","147"]
["مروحة","الضغط الاستاتيكي الخارجي","عالٍ","باسكال","53","96","126","120"]
["","","منخفض","باسكال","25","61","92","69"]
["الأبعاد","الوحدة","الارتفاع","mm","285","305","378","378"]
["","","العرض","mm","1020","1325","1388","1588"]
["","","العمق","mm","600","638","541","541"]
["الوزن","الوحدة","","kg","35","47","50","56"]
["مروحة","الضغط الاستاتيكي الخارجي","الإسمي","باسكال","38","78","109","90"]
["مستوى طاقة الصوت","التبريد","","dBA","64","76","76","78"]
["","التدفئة","","dBA","64","76","76","78"]
["Sound pressure level","Cooling","Super high","dBA","44","55","53","55"]
["","","High","dBA","41","51","52","53"]
["","","Nom.","dBA","38","48","50","50"]
["","","Low","dBA","34","45","47","47"]
["","Heating","High","dBA","41","51","52","53"]
["","","Nom.","dBA","38","48","50","50"]
["","","Low","dBA","34","45","47","47"]
["وصلات الأنابيب","سائل","القطر الخارجي","mm","9.52","9.52","9.52","9.52"]
["","غاز","القطر الخارجي","mm","15.88","15.88","15.88","15.88"]
["وحدة التزويد بالطاقة","الاسم","","","V1","V1","V1","V1"]
["","الطور","","","1~","1~","1~","1~"]
["Power supply","Frequency","","Hz","50","50","50","50"]
["","Voltage","","V","230","230","230","230"]