{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-A"]
[]
[]
[]
[]
["","","","","ABQ100AV1","ABQ125AV1","ABQ140AV1","ABQ71AV1"]
["Sound pressure level","Heating","High","dBA","51","52","53","41"]
["","","Nom.","dBA","48","50","50","38"]
["","","Low","dBA","45","47","47","34"]
["","Cooling","Super high","dBA","55","53","55","44"]
["","","Low","dBA","45","47","47","34"]
["","","High","dBA","51","52","53","41"]
["","","Nom.","dBA","48","50","50","38"]
["Piping connections","Liquid","القطر الخارجي","mm","9.52","9.52","9.52","9.52"]
["","غاز","القطر الخارجي","mm","15.88","15.88","15.88","15.88"]
["Sound power level","التبريد","","dBA","76","76","78","64"]
["","التدفئة","","dBA","76","76","78","64"]
["Dimensions","Unit","العرض","mm","1,325","1,388","1,588","1,020"]
["","","العمق","mm","638","541","541","600"]
["","","الارتفاع","mm","305","378","378","285"]
["الوزن","الوحدة","","kg","47.0","50.0","56.0","35.0"]
["Fan","External static pressure","عالٍ","باسكال","96","126","120","53"]
["","","الإسمي","باسكال","78","109","90","38"]
["","","منخفض","باسكال","61","92","69","25"]
["","","Super high","باسكال","118","147","147","78"]
["Power supply","الطور","","","1~","1~","1~","1~"]
["","الاسم","","","V1","V1","V1","V1"]
["","Frequency","","Hz","50","50","50","50"]
["","Voltage","","V","230","230","230","230"]