{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-B"]
[]
[]
[]
[]
["","","","","","ADEQ71B2VEB","ADEQ100B2VEB","ADEQ125B2VEB"]
["مروحة","الضغط الاستاتيكي الخارجي","","عالٍ","باسكال","150","150","150"]
["Cooling capacity","Total capacity","","Nom.","kW","6.8","9.5","12.1"]
["استطاعة التدفئة","الاستطاعة الإجمالية","","الإسمي","kW","7.50","10.80","13.50"]
["الغلاف","اللون","","","","Unpainted","Unpainted","Unpainted"]
["","المادة","","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["الأبعاد","الوحدة","","الارتفاع","mm","245","245","245"]
["","","","العرض","mm","1000","1400","1400"]
["","","","العمق","mm","800","800","800"]
["الوزن","الوحدة","","","kg","35","46","46"]
["Fan","Air flow rate","Cooling","High","m³/min","18","29","34"]
["","","","Nom.","m³/min","15","26","29"]
["","","","Low","m³/min","12.5","23","23.5"]
["","","Heating","High","m³/min","18","29","34"]
["","","","Nom.","m³/min","15","26","29"]
["","","","Low","m³/min","12.5","23","23.5"]
["مروحة","الضغط الاستاتيكي الخارجي","","الإسمي","باسكال","30","40","50"]
["مستوى طاقة الصوت","التبريد","","","dBA","56","58","62"]
["Sound pressure level","Cooling","","High","dBA","30","34","37"]
["","","","Nom.","dBA","28","32","35"]
["","","","Low","dBA","25","30","32"]
["","Heating","","High","dBA","31","36","38"]
["","","","Nom.","dBA","28","33","35"]
["","","","Low","dBA","25","30","32"]
["سائل تبريد","GWP","","","","2,087.5","2,087.5","2,087.5"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","15.9","15.9","15.9"]
["","التصريف","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["ارتفاع الصرف","mm","","","","625","625","625"]
["Standard Accessories","دليل التركيب","","","","1","1","1"]
["","حلقة للدعامة الحاملة","","","","8","8","8"]
["","دليل التشغيل","","","","1","1","1"]
["","مشابك","","","","4","4","4"]
["","خرطوم الصرف","","","","1","1","1"]
["","عازل لأدوات التثبيت","","","","2","2","2"]
["","مشبك معدني لخرطوم الصرف","","","","1","1","1"]
["","مسامير لولبية","","","","40","40","40"]
["","لبادة مانعة للتسريب","","","","5","5","5"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(1) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(1) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت."]