{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":9,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C"]
[]
[]
[]
[]
["","","","","","AHQ71CV1","AHQ100CV1","AHQ125CV1","AHQ140CV1"]
["Power input","Heating","","Nom.","kW","0.106","0.149"]
["","Cooling","","Nom.","kW","0.106","0.149"]
["مروحة","الضغط الاستاتيكي الخارجي","","عالٍ","باسكال","0","0","0","0"]
["","","","منخفض","باسكال","0","0","0","0"]
["Cooling capacity","Total capacity","","Nom.","kW","","","12.10","13.00"]
["استطاعة التدفئة","الاستطاعة الإجمالية","","الإسمي","kW","","","13.5","15.5"]
["الغلاف","اللون","","","","أبيض","أبيض","أبيض","أبيض"]
["","المادة","","","","Galvanised steel","Galvanised steel"]
["الأبعاد","الوحدة","","الارتفاع","mm","260","260","260","285"]
["","","","العرض","mm","1320","1538","1790","1900"]
["","","","العمق","mm","634","634","634","680"]
["الوزن","الوحدة","","","kg","38","45","65","70"]
["Fan","Air flow rate","Cooling","High","m³/min","23.8","31.1","34.4","43.9"]
["","","","Nom.","m³/min","21.3","27.8","31","39"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","","","31","39"]
["Fan","Air flow rate","Cooling","Low","m³/min","18.9","24.8","27.2","28.3"]
["","","Heating","High","m³/min","23.8","31.1","34.4","43.9"]
["","","","Nom.","m³/min","21.3","27.8","30.6","39.1"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","","","30.6","39.1"]
["Fan","Air flow rate","Heating","Low","m³/min","18.9","24.8","27.2","28.3"]
["مروحة","الضغط الاستاتيكي الخارجي","","الإسمي","باسكال","0","0","0","0"]
["مستوى طاقة الصوت","التبريد","","","dBA","59","64","65","71"]
["","التدفئة","","","dBA","62","64","65","71"]
["Sound pressure level","Cooling","","High","dBA","49","52","52","56"]
["","","","Nom.","dBA","48","47"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","","","50","53"]
["Sound pressure level","Cooling","","Low","dBA","46","46","49","46"]
["","Heating","","High","dBA","49","52","52","56"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","","","50","53"]
["Sound pressure level","Heating","","Nom.","dBA","48","47"]
["","","","Low","dBA","46","46","49","46"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","9.52","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","15.88","15.88","15.9","15.9"]
["","التصريف","","","","19.05","19.05"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","ARCWLA","ARCWLA","ARCWLA","ARCWLA"]
["","جهاز تحكم عن بُعد سلكي","","","","ARCWB","ARCWB"]
["Standard Accessories","دليل التركيب","","","","دليل التركيب","دليل التركيب"]
["","جهاز تحكم عن بعد لاسلكي","","","","جهاز تحكم عن بعد لاسلكي","جهاز تحكم عن بعد لاسلكي"]
["","بطارية","","","","بطارية","بطارية"]
["","أنبوب الصرف","","","","أنبوب الصرف","أنبوب الصرف"]
["","برغي لجهاز التحكم عن بعد اللاسلكي","","","","برغي لجهاز التحكم عن بعد اللاسلكي","برغي لجهاز التحكم عن بعد اللاسلكي"]
["","قلب فرّيتي","","","","قلب فرّيتي","قلب فرّيتي"]
["","دليل التركيب (قلب فرّيتي)","","","","دليل التركيب (قلب فرّيتي)","دليل التركيب (قلب فرّيتي)"]
["","مخطط التوصيل السلكي الخارجي","","","","مخطط التوصيل السلكي الخارجي","مخطط التوصيل السلكي الخارجي"]
["","دليل التشغيل","","","","دليل التشغيل","دليل التشغيل"]
["","خرطوم الصرف","","","","خرطوم الصرف","خرطوم الصرف"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1"]
["","الطور","","","","1~","1~"]
["Power supply","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]