{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-M9"]
[]
[]
[]
[]
["","","","","","ARXM25M3V1B9","ARXM35M3V1B9","ARXM50M3V1B9"]
["الأبعاد","الوحدة","","الارتفاع","mm","550","550","735"]
["","","","العرض","mm","765","765","825"]
["","","","العمق","mm","285","285","300"]
["الوزن","الوحدة","","","kg","32","32","47"]
["Compressor","Type","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-10","-10","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","46","46","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","10","10","10"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","18","18","18"]
["Sound pressure level","Cooling","","Nom.","dBA","46","49","48"]
["","Heating","","Nom.","dBA","47","49","49"]
["سائل تبريد","النوع","","","","R-32","R-32","R-32"]
["","السعة","","","kg","0.76","0.76","1.40"]
["","السعة","","","tCO2Eq","0.52","0.52","0.95"]
["","GWP","","","","675.0","675.0","675"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","20.0","20.0","30"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","20.0","20.0","20"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - يحتوي على غازات الاحتباس الحراري المفلورة","(1) - يحتوي على غازات الاحتباس الحراري المفلورة","(1) - انظر الرسم المنفصل لنطاق التشغيل"]