{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXP-M"]
[]
[]
[]
[]
["","","","","","ARXP20M5V1B","ARXP25M5V1B","ARXP35M5V1B"]
["الأبعاد","الوحدة","","الارتفاع","mm","550","550","550"]
["","","","العرض","mm","658","658","658"]
["","","","العمق","mm","275","275","275"]
["الوزن","الوحدة","","","kg","26","26","28"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-10","-10","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","48","48","48"]
["Sound pressure level","Cooling","","High","dBA","46","46","48"]
["","Heating","","High","dBA","47","47","48"]
["سائل تبريد","النوع","","","","R-32","R-32","R-32"]
["","السعة","","","kg","0.55","0.55","0.70"]
["","السعة","","","tCO2Eq","0.37","0.37","0.48"]
["","GWP","","","","675.0","675.0","675.0"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","15","15","15"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","12","12","12"]
["Standard Accessories","دليل التركيب","","","","1","1","1"]
["","ملصق الشحن بسائل التبريد","","","","1","1","1"]
["","ملصقات متعددة اللغات حول غازات الدفيئة المفلورة","","","","1","1","1"]
["","تدابير السلامة الوقائية العامة","","","","1","1","1"]
["","سدادة المصرف","","","","1","1","1"]
["نطاق كفاءة استخدام الطاقة","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","","(3) - يحتوي على غازات الاحتباس الحراري المفلورة","(3) - يحتوي على غازات الاحتباس الحراري المفلورة","(3) - يحتوي على غازات الاحتباس الحراري المفلورة"]