{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":15,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-G"]
[]
[]
[]
[]
["","","","","","ARXS20G3V1B","ARXS20G4V1B","ARXS25G3V1B","ARXS25G4V1B","ARXS35G3V1B","ARXS35G4V1B","ARXS42G2V1B","ARXS42G3V1B","ARXS50G2V1B","ARXS50G3V1B"]
["Sound pressure level","Heating","","High","dBA","47","47","47","47","48","48","48","48"]
["","Cooling","","High","dBA","46","46","46","46","48","48","48","48"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1","1","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","1.7","1.7","2.1","2.1","2.5","2.5","2.7","2.7"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","0.8","0.8","1.0","1.0","1.2","1.2","1.3","1.3"]
["","النوع","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Piping connections","Level difference","IU - OU","Max.","م","15","15","15","15","15","15","15","15"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["Sound power level","التبريد","","","dBA","","","","","","","63"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","mm","765","765","765","765","765","765","765","765"]
["","","","العمق","mm","285","285","285","285","285","285","285","285"]
["","","","الارتفاع","mm","550","550","550","550","550","550","550","550"]
["الوزن","الوحدة","","","kg","32","32","34","34","34","34","39","39"]
["Power supply","الطور","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting"]
["","","","","","(2) - يحتوي على غازات الاحتباس الحراري المفلورة","(2) - يحتوي على غازات الاحتباس الحراري المفلورة","(2) - يحتوي على غازات الاحتباس الحراري المفلورة","(2) - يحتوي على غازات الاحتباس الحراري المفلورة","(2) - يحتوي على غازات الاحتباس الحراري المفلورة","(2) - يحتوي على غازات الاحتباس الحراري المفلورة","(2) - يحتوي على غازات الاحتباس الحراري المفلورة","(2) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["Standard Accessories","سدادة المصرف","","","","1","1"]
["الأبعاد","الوحدة","","الارتفاع","mm","","","","","","","","","735","735"]
["","","","العرض","mm","","","","","","","","","825","825"]
["","","","العمق","mm","","","","","","","","","300","300"]
["الوزن","الوحدة","","","kg","","","","","","","","","48","48"]
["ضاغط","نوع","","","","","","","","","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","","","","","","","","","-10","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","","","","","","","","","46","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","","","","","","","","","-15","-15"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","","","","","","","","","20","18"]
["Sound pressure level","Cooling","","High","dBA","","","","","","","","","48","48"]
["","Heating","","High","dBA","","","","","","","","","48","48"]
["سائل تبريد","النوع","","","","","","","","","","","","R-410A","R-410A"]
["","السعة","","","kg","","","","","","","","","1.7","1.7"]
["","السعة","","","tCO2Eq","","","","","","","","","3.5","3.5"]
["","GWP","","","","","","","","","","","","2087.5","2087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","","","","","","","","","30","30"]
["Piping connections","Additional refrigerant charge","","","kg/m","","","","","","","","","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","","","","","","","","","20","20"]
["وحدة التزويد بالطاقة","الطور","","","","","","","","","","","","1~","1~"]
["Power supply","Frequency","","","Hz","","","","","","","","","50","50"]
["","Voltage","","","V","","","","","","","","","220-240","220-240"]