{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":10,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L"]
[]
[]
[]
[]
["","","","","","ARXS25L2V1B","ARXS35L2V1B","ARXS50L2V1B","ARXS60L2V1B","ARXS71L2V1B"]
["المروحة","معدل تدفق الهواء","التبريد","منخفض جداً","m³/min","30.1","30.1","48.9"]
["","","التدفئة","منخفض جداً","m³/min","25.6","25.6","43.1"]
["مستوى طاقة الصوت","التدفئة","","","dBA","","","","62","65"]
["","التبريد","","","dBA","","","","62","65"]
["المروحة","معدل تدفق الهواء","التبريد","منخفض جداً","cfm","1063","1063","1727"]
["","","التدفئة","منخفض جداً","cfm","904","904","1522"]
["الأبعاد","الوحدة","","الارتفاع","mm","550","550","735","735","735"]
["","","","العرض","mm","765","765","825","825","825"]
["","","","العمق","mm","285","285","300","300","300"]
["الوزن","الوحدة","","","kg","34","34","47","47","47"]
["محرك المروحة","السرعة","التبريد","منخفض جداً","rpm","780","780","670"]
["","","التدفئة","منخفض جداً","rpm","740","740","670"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","10","10","10","-10","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","46","46","46","46","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-15","-15","-15","-15","-15"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","18","18","18","18","18"]
["Sound pressure level","Cooling","","High","dBA","46","48","48"]
["","","","Nom.","dBA","","","","49","52"]
["","Heating","","High","dBA","47","48","48"]
["","","","Nom.","dBA","","","","49","52"]
["سائل تبريد","النوع","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","السعة","","","kg","1.0","1.2","1.7","1.50","1.70"]
["","السعة","","","tCO2Eq","2.1","2.5","3.5"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","20","20","30","30","30"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","15","15","20","20.0","20.0"]
["Standard Accessories","دليل التركيب","","","","1","1","1","1","1"]
["","ملصق الشحن بسائل التبريد","","","","1","","","1","1"]
["","ملصقات متعددة اللغات حول غازات الدفيئة المفلورة","","","","1","","","1","1"]
["","سدادة المصرف","","","","1","1","1","1","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-230-240","220-230-240"]
["Notes","","","","","(1) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها.","(1) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها.","(1) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها."]
["","","","","","(2) - 220 فولت","(2) - 220 فولت","(2) - 220 فولت"]
["","","","","","(3) - 230 فولت","(3) - 230 فولت","(3) - 230 فولت"]
["","","","","","(4) - 240 فولت","(4) - 240 فولت","(4) - 240 فولت"]
["","","","","","(5) - يحتوي على غازات الاحتباس الحراري المفلورة","(5) - يحتوي على غازات الاحتباس الحراري المفلورة","(5) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["","","","","","","","","(1) - يحتوي على غازات الاحتباس الحراري المفلورة","(1) - يحتوي على غازات الاحتباس الحراري المفلورة"]