{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A / ARXF-F"]
[]
[]
[]
[]
["","","","","ATXF50A2V1B / ARXF50F5V1B"]
["Outdoor unit","","","","ARXF50F5V1B"]
["Cooling capacity","Min.","","kW","1.3"]
["","Nom.","","kW","5"]
["","Max.","","kW","5.3"]
["Heating capacity","Min.","","kW","1.43"]
["","Nom.","","kW","5.4"]
["","Max.","","kW","6.13"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","3.27"]
["","عامل الأداء","","","3.71"]
["","استهلاك الطاقة السنوي","","kWh","271"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","A"]
["","","تدفئة","","A"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A++"]
["","الاستطاعة","Pdesign","kW","5"]
["","SEER","","","6.45"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","271"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A+"]
["","الاستطاعة","Pdesign","kW","3.8"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","4.07"]
["","Pdh استطاعة التدفئة عند -10°","","kW","3.24"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","1309"]
["نطاق كفاءة استخدام الطاقة","","","","A+++ ~ D"]
["Notes","","","","(1) - تستند استطاعات التبريد الإسمية إلى: درجة الحرارة الداخلية: 27‏°CDB، و19‏°CWB؛ درجة الحرارة الخارجية: 35‏°CDB، طول أنابيب سائل التبريد المكافئ: 5م، فرق المستوى: 0م. بيانات السلسلة عالية الفعالية، بشهادة Eurovent"]
["","","","","(2) - تستند استطاعات التدفئة الإسمية إلى: درجة الحرارة الداخلية: 20‏°CDB، درجة الحرارة الخارجية: 7‏°CDB، و6°CWB، طول أنابيب سائل التبريد المكافئ: 5م، فرق المستوى: 0م. بيانات سلسلة الفعالية القياسية"]
["","","","","(3) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]