{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A"]
[]
[]
[]
[]
["","","","","","ATXF20A5V1B","ATXF25A5V1B","ATXF35A5V1B","ATXF50A2V1B","ATXF60A2V1B","ATXF71A2V1B"]
["Power input","Cooling","","Nom.","kW","0.019","0.019","0.032","0.029","0.032","0.032"]
["","Heating","","Nom.","kW","0.02","0.02","0.032","0.032","0.035","0.035"]
["الغلاف","اللون","","","","أبيض","أبيض","أبيض","أبيض","أبيض","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","286","286","286","295","295","295"]
["","","","العرض","mm","770","770","770","990","990","990"]
["","","","العمق","mm","225","225","225","263","263","263"]
["الوزن","الوحدة","","","kg","8.5","8.5","9","13.5","13.5","13.5"]
["Fan","Air flow rate","Cooling","High","m³/min","10.1","10.1","11.5","16.8","17.3","17.3"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","8.1","8.1","8.3","14.4","14.8","14.8"]
["Fan","Air flow rate","Cooling","Low","m³/min","6.1","6.1","6.3","11.9","12.2","12.2"]
["","","","Silent operation","m³/min","4.4","4.4","4.5","10.5","10.7","10.7"]
["","","Heating","High","m³/min","10.3","10.3","11.5","17.3","17.9","17.9"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","8.6","8.6","9","14.8","15.8","15.8"]
["Fan","Air flow rate","Heating","Low","m³/min","6.7","6.7","7","12.2","12.8","12.8"]
["","","","Silent operation","m³/min","5.3","5.3","5.3","10.7","11.3","11.3"]
["مستوى طاقة الصوت","التبريد","","","dBA","55","55","58","59","60","62"]
["","التدفئة","","","dBA","55","55","58","61","62","62"]
["Sound pressure level","Cooling","","High","dBA","40","40","43","43","45","46"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","33","33","34","39","41","42"]
["Sound pressure level","Cooling","","Low","dBA","26","26","27","34","36","37"]
["","","","Silent operation","dBA","20","20","20","31","33","34"]
["","Heating","","High","dBA","40","40","40","42","44","45"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","34","34","35","38","40","41"]
["Sound pressure level","Heating","","Low","dBA","28","28","29","33","35","36"]
["","","","Silent operation","dBA","21","21","21","30","32","33"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.5","9.5","9.5","12.7","12.7","12.7"]
["","التصريف","","","","18","18","18","18","18","18"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["","جهاز تحكم عن بُعد سلكي","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standard Accessories","دليل التركيب","","","","1","1","1","1","1","1"]
["","بطاريات جافة قياس AAA","","","","2","2","2","2","2","2"]
["","دليل التشغيل","","","","1","1","1","1","1","1"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","","2","2","2","2","2","2"]
["","جهاز تحكم عن بعد بالأشعة تحت الحمراء","","","","1","1","1","1","1","1"]
["","لوح التثبيت","","","","1","1","1","1","1","1"]
["","حامل جهاز التحكم عن بعد","","","","1","1","1","1","1","1"]
["نطاق كفاءة استخدام الطاقة","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["وحدة التزويد بالطاقة","الاسم","","","","","","","V1","V1","V1"]
["","الطور","","","","1~","1~","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]