{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-E"]
[]
[]
[]
[]
["","","","","","ATXF20E5V1B","ATXF25E5V1B","ATXF35E5V1B","ATXF42E5V1B"]
["Power input","Cooling","","Nom.","kW","0.023","0.023","0.029","0.040"]
["","Heating","","Nom.","kW","0.023","0.023","0.029","0.040"]
["الغلاف","اللون","","","","أبيض","أبيض","أبيض","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","286","286","286","286"]
["","","","العرض","mm","770","770","770","770"]
["","","","العمق","mm","225","225","225","225"]
["الوزن","الوحدة","","","kg","8","8","8.5","9.00"]
["Fan","Air flow rate","Cooling","High","m³/min","9.8","10","11.5","12.6"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","8","8","8","9"]
["Fan","Air flow rate","Cooling","Low","m³/min","6","6.2","6.4","6.9"]
["","","","Silent operation","m³/min","4.3","4.3","4.4","4.9"]
["","","Heating","High","m³/min","10.4","10.4","11.9","12.8"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","8.3","8.4","8.6","8.8"]
["Fan","Air flow rate","Heating","Low","m³/min","6.2","6.4","6.5","6.7"]
["","","","Silent operation","m³/min","5.3","5.3","5.3","5.2"]
["مستوى طاقة الصوت","التبريد","","","dBA","53","54","54","59.0"]
["","التدفئة","","","dBA","55","55","56","59.0"]
["Sound pressure level","Cooling","","High","dBA","39","40","43","45.0"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","33","33","34","36.0"]
["Sound pressure level","Cooling","","Low","dBA","25","26","27","30.0"]
["","","","Silent operation","dBA","20","20","20","22.0"]
["","Heating","","High","dBA","39","40","40","44.0"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","34","34","35","34.0"]
["Sound pressure level","Heating","","Low","dBA","28","28","29","28.0"]
["","","","Silent operation","dBA","21","21","21","22.0"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6","6","6","6"]
["","غاز","","القطر الخارجي","mm","9.5","9.5","9.5","9.50"]
["","التصريف","","","","18","18","18","18"]
["أنظمة التحكم","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["أنظمة التحكم","جهاز تحكم عن بُعد سلكي","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~","1~"]
["Power supply","Power supply-=-Frequency","","Frequency","","50","50","50","50"]
["","Power supply-=-Voltage","","Voltage","","220-440","220-440","220-440","220-440"]