{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-F"]
[]
[]
[]
[]
["","","","","","ATXF50F5V1B"]
["Power input","Cooling","","Nom.","kW","0.04"]
["","Heating","","Nom.","kW","0.04"]
["الغلاف","اللون","","","","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","286"]
["","","","العرض","mm","770"]
["","","","العمق","mm","225"]
["الوزن","الوحدة","","","kg","9"]
["Fan","Air flow rate","Cooling","High","m³/min","12.6"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","9"]
["Fan","Air flow rate","Cooling","Low","m³/min","7.2"]
["","","","Silent operation","m³/min","6.4"]
["","","Heating","High","m³/min","12.8"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","9.6"]
["Fan","Air flow rate","Heating","Low","m³/min","7.2"]
["","","","Silent operation","m³/min","6.4"]
["مستوى طاقة الصوت","التبريد","","","dBA","59"]
["","التدفئة","","","dBA","59"]
["Sound pressure level","Cooling","","High","dBA","45"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","39"]
["Sound pressure level","Cooling","","Low","dBA","34"]
["","","","Silent operation","dBA","31"]
["","Heating","","High","dBA","44"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","38"]
["Sound pressure level","Heating","","Low","dBA","33"]
["","","","Silent operation","dBA","30"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6"]
["","غاز","","القطر الخارجي","mm","12.7"]
["","التصريف","","","","18"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","ARC480A93"]
["","جهاز تحكم عن بُعد سلكي","","","","BRC073A1"]
["Standard Accessories","ATXF50F5V1B","","","","1"]
["","Installation manual","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Infrared remote control","","","","1"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~"]
["Power supply","Frequency","","","Hz","50"]
["","Voltage","","","V","220-440"]
["Notes","","","","","(1) - التبريد: درجة الحرارة الداخلية 27 درجة مئوية للبويصلة الجافة، 19 درجة مئوية للبويصلة الرطبة؛ درجة الحرارة الخارجية: 35 درجة مئوية للبويصلة الجافة؛ الطول المكافئ للمواسير: 5 متر؛ فرق المستوى: 0 متر"]
["","","","","","(2) - التدفئة: درجة الحرارة الداخلية 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة؛ الطول المكافئ للمواسير: 5 متر (أفقي)"]
["","","","","","(3) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]