{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R / ARXM-R9"]
[]
[]
[]
[]
["","","","","ATXM25R2V1B / ARXM25R5V1B9","ATXM25R5V1B / ARXM25R5V1B9","ATXM35R2V1B / ARXM35R5V1B9","ATXM35R5V1B / ARXM35R5V1B9"]
["Cooling capacity","Min.","","kW","","","1.40"]
["","Max.","","kW","","","4.00"]
["","Nom.","","kW","","","3.40"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","","","402"]
["","نسبة فعالية استهلاك الطاقة","","","","","4.23"]
["","عامل الأداء","","","","","4.04"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","","A"]
["","","تدفئة","","","","A"]
["Heating capacity","Nom.","","kW","","","4.00"]
["","Min.","","kW","","","1.40"]
["","Max.","","kW","","","5.20"]
["Notes","","","","","","(1) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","","","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م."]
["","","","","","","(4) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]
["Cooling capacity","Min.","","kW","1.30","1.30","","1.40"]
["","Nom.","","kW","2.50","2.50","","3.40"]
["","Max.","","kW","3.20","3.20","","4.00"]
["Heating capacity","Min.","","kW","1.30","1.30","","1.40"]
["","Nom.","","kW","2.80","2.80","","4.00"]
["","Max.","","kW","4.70","4.70","","5.20"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","4.50","4.50","","4.23"]
["","عامل الأداء","","","5.00","5.00","","4.04"]
["","استهلاك الطاقة السنوي","","kWh","278","278","","402"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","","A"]
["","","تدفئة","","A","A","","A"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A+++","A+++","","A+++"]
["","الاستطاعة","Pdesign","kW","2.50","2.50","","3.40"]
["","SEER","","","8.55","8.55","","8.55"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","102","102","","139"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A+++","A+++","","A+++"]
["","الاستطاعة","Pdesign","kW","2.40","2.40","","2.50"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","5.10","5.10","","5.10"]
["","Pdh استطاعة التدفئة عند -10°","","kW","2.30","2.30","","2.35"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","659","659","","686"]
["نطاق كفاءة استخدام الطاقة","","","","A+++ ~ D","A+++ ~ D","","A+++ ~ D"]