{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXS-G"]
[]
[]
[]
[]
["","","","","ATXS20G2V1B","ATXS25G2V1B","ATXS35G2V1B","ATXS50G2V1B"]
["Sound pressure level","Heating","High","dBA","38","39","42","44"]
["","","Silent operation","dBA","25","25","26","31"]
["","","Low","dBA","28","28","29","34"]
["","Cooling","Silent operation","dBA","22","22","23","31"]
["","","Low","dBA","25","25","26","34"]
["","","High","dBA","38","38","42","43"]
["","","Nom.","dBA","33","34","36","39"]
["","Cooling","Nom.","dBA","32","32","34","39"]
["Standard Accessories","مرشح تنقية الهواء بالتحفيز الضوئي وأباتيت التيتانيوم","","","2","2","2","2"]
["","دليل التشغيل","","","1","1","1","1"]
["","دليل التركيب","","","1","1","1","1"]
["","جهاز تحكم عن بعد لاسلكي","","","1","1","1","1"]
["","البطاريات","","","2","2","2","2"]
["","حامل جهاز التحكم عن بعد","","","1","1","1","1"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","2","2","2","2"]
["","لوح التثبيت","","","1","1","1","1"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35","6.35","6.35","6.35"]
["","غاز","القطر الخارجي","mm","9.5","9.5","9.5","12.7"]
["","Drain","","","18","18","18","18"]
["Power input","Cooling","Nom.","kW","0.018 (1), 0.018 (2), 0.018 (3)","0.018 (1), 0.018 (2), 0.018 (3)","0.026 (1), 0.026 (2), 0.026 (3)","0.026 (1), 0.026 (2), 0.026 (3)"]
["","Heating","Nom.","kW","0.021 (1), 0.021 (2), 0.021 (3)","0.021 (1), 0.021 (2), 0.021 (3)","0.028 (1), 0.028 (2), 0.280 (3)","0.032 (1), 0.032 (2), 0.032 (3)"]
["Sound power level","التبريد","","dBA","54","54","59","60"]
["","التدفئة","","dBA","54","55","58","60"]
["Dimensions","Unit","العرض","mm","800","800","800","800"]
["","","العمق","mm","215","215","215","215"]
["","","الارتفاع","mm","295","295","295","295"]
["الغلاف","اللون","","","White","White","White","White"]
["الوزن","الوحدة","","kg","9","9","10","10"]
["Power supply","الطور","","","1~","1~","1~","1~"]
["","Frequency","","Hz","50","50","50","50"]
["","الاسم","","","V1","V1","V1","V1"]
["","Voltage","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت"]
["","","","","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت"]
["","","","","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت"]
["","","","","(4) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء","(4) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء","(4) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء","(4) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء"]