{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXS-K / ARXS-L3"]
[]
[]
[]
[]
["","","","","ATXS25K3V1B / ARXS25L3V1B","ATXS25K2V1B / ARXS25L3V1B","ATXS35K3V1B / ARXS35L3V1B","ATXS35K2V1B / ARXS35L3V1B"]
["Cooling capacity","Min.","","kW","","","1.4"]
["","Max.","","kW","","","4.0"]
["","Nom.","","kW","2.5 (2)","","3.5 (2)"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35","","6.35"]
["","غاز","القطر الخارجي","mm","9.5","","9.5"]
["","Drain","OD","mm","18","","18"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","301","","473"]
["","نسبة فعالية استهلاك الطاقة","","","4.15 (1)","","3.70 (1)"]
["","عامل الأداء","","","4.52 (1)","","4.76 (1)"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","","A"]
["","","تدفئة","","A","","A"]
["Heating capacity","Nom.","","kW","2.8 (2)","","4.00 (2)"]
["","Min.","","kW","1.3","","1.4"]
["","Max.","","kW","4.7","","5.2"]
["Notes","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]
["","","","","(3) - 220 فولت","","(3) - 220 فولت"]
["","","","","(4) - 230 فولت","","(4) - 230 فولت"]
["","","","","(5) - 240 فولت","","(5) - 240 فولت"]
["Outdoor unit","","","","","ARXS25L3","","ARXS35L3"]
["Cooling capacity","Nom.","","kW","","2.5","","3.5"]
["Heating capacity","Nom.","","kW","","2.8","","4.00"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","","4.15","","3.70"]
["","عامل الأداء","","","","4.52","","4.76"]
["","استهلاك الطاقة السنوي","","kWh","","301","","473"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","","A","","A"]
["","","تدفئة","","","A","","A"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","","A++","","A++"]
["","الاستطاعة","Pdesign","kW","","2.50","","3.50"]
["","SEER","","","","7.51","","7.10"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","117","","173"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","","A++","","A++"]
["","الاستطاعة","Pdesign","kW","","2.50","","3.60"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","","4.68","","4.61"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","747","","1094"]