{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":13,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXS-K"]
[]
[]
[]
[]
["","","","","","ATXS20K2V1B","ATXS20K3V1B","ATXS25K2V1B","ATXS25K3V1B","ATXS35K2V1B","ATXS35K3V1B","ATXS50K2V1B","ATXS50K3V1B"]
["Sound pressure level","Heating","","High","dBA","","","","","","","47","47"]
["","","","Silent operation","dBA","","","","","","","24","24"]
["","","","Low","dBA","","","","","","","34","34"]
["","Cooling","","Silent operation","dBA","","","","","","","23","23"]
["","","","Low","dBA","","","","","","","34","34"]
["","","","High","dBA","","","","","","","46","46"]
["","","","Nom.","dBA","","","","","","","40","40"]
["","Cooling","","Nom.","dBA","","","","","","","40","40"]
["Standard Accessories","دليل التركيب","","","","","","","","","","1","1"]
["","دليل التشغيل","","","","","","","","","","1","1"]
["","جهاز تحكم عن بعد بالأشعة تحت الحمراء","","","","","","","","","","1","1"]
["","البطاريات","","","","","","","","","","2","2"]
["","حامل جهاز التحكم عن بعد","","","","","","","","","","1","1"]
["","لوح التثبيت","","","","","","","","","","1","1"]
["","مرشح تنقية الهواء بالتحفيز الضوئي وأباتيت التيتانيوم","","","","","","","","","","2","2"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","","","","","","","","2","2"]
["أنظمة التحكم","Infrared remote control","","","","","","","","","","","ARC466A9"]
["Piping connections","Liquid","","القطر الخارجي","mm","","","","","","","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","","","","","","","12.7","12.7"]
["","Drain","","","","","","","","","","18","18"]
["Power input","Cooling","","Nom.","kW","","","","","","","0.026 (2), 0.026 (3), 0.026 (4)"]
["","Heating","","Nom.","kW","","","","","","","0.032 (2), 0.032 (3), 0.032 (4)"]
["Sound power level","التبريد","","","dBA","","","","","","","60","60"]
["","التدفئة","","","dBA","","","","","","","60","60"]
["Dimensions","Unit","","العرض","mm","","","","","","","900","900"]
["","","","العمق","mm","","","","","","","215","215"]
["","","","الارتفاع","mm","","","","","","","298","298"]
["الغلاف","اللون","","","","","","","","","","White","White"]
["الوزن","الوحدة","","","kg","","","","","","","11","11"]
["Power supply","الطور","","","","","","","","","","1~","1~"]
["","Frequency","","","Hz","","","","","","","50","50"]
["","الاسم","","","","","","","","","","V1","V1"]
["","Voltage","","","V","","","","","","","220-240","220-240"]
["Notes","","","","","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها.","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء"]
["","","","","","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 220 فولت","(2) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها."]
["","","","","","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 230 فولت","(3) - 220 فولت"]
["","","","","","","","","","","","(4) - 240 فولت","(4) - 230 فولت"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","7.0","7.0","7.0","7.0","8.5","8.5"]
["Sound pressure level","Cooling","","Nom.","dBA","32","32","33","33","37","37"]
["Fan","Air flow rate","Heating","Nom.","m³/min","8.0","8.0","8.0","8.0","9.3","9.3"]
["Power input","Cooling","","Nom.","kW","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","","0.040 (3) (2) (4), 0.040 (3) (2) (4), 0.040 (3) (2) (4)","","0.026 (3) (2) (4), 0.026 (3) (2) (4), 0.026 (3) (2) (4)"]
["","Heating","","Nom.","kW","0.040 (1) (3) (2), 0.040 (1) (3) (2), 0.040 (1) (3) (2)","","0.040 (2) (4) (3), 0.040 (2) (4) (3), 0.040 (2) (4) (3)","","0.028 (3) (2), 0.028 (3) (2), 0.280 (4)"]
["الغلاف","اللون","","","","أبيض","أبيض","أبيض","أبيض","أبيض","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","289","289","289","289","298","298"]
["","","","العرض","mm","780","780","780","780","900","900"]
["","","","العمق","mm","215","215","215","215","215","215"]
["الوزن","الوحدة","","","kg","8","8","8","8","11","11"]
["Fan","Air flow rate","Cooling","High","m³/min","9.1","9.1","9.1","9.1","11.2","11.2"]
["","","","Low","m³/min","5.0","5.0","5.0","5.0","5.8","5.8"]
["","","","Silent operation","m³/min","3.9","3.9","3.9","3.9","4.1","4.1"]
["","","Heating","High","m³/min","10.0","10.0","10.0","10.0","12.1","12.1"]
["","","","Low","m³/min","6.0","6.0","6.0","6.0","6.5","6.5"]
["","","","Silent operation","m³/min","4.3","4.3","4.3","4.3","4.2","4.2"]
["مستوى طاقة الصوت","التبريد","","","dBA","54","56","58","58","59","59"]
["","التدفئة","","","dBA","56","56","58","58","59","59"]
["Sound pressure level","Cooling","","High","dBA","40","40","41","41","45","45"]
["","","","Low","dBA","24","24","25","25","29","29"]
["","","","Silent operation","dBA","19","19","19","19","19","19"]
["","Heating","","High","dBA","40","40","41","41","45","45"]
["","","","Low","dBA","27","27","27","27","29","29"]
["","","","Silent operation","dBA","19","19","19","19","19","19"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.5","9.5","9.5","9.5","9.5","9.5"]
["","التصريف","","","","18","18","18","18","18","18"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","Operation manual","","","","1","1","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1"]
["","Titanium apatite photocatalytic air purification filter","","","","2","2","2","2","2","2"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1","V1","V1","V1","V1"]
["","الطور","","","","1~","1~","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Sound pressure level","Heating","","Nom.","dBA","","34","34","34","39","39"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","","ARC466A6","","ARC466A6","","ARC466A9"]
["Standard Accessories","Batteries","","","","","","","","2","2"]
["Notes","","","","","","","","","","","","(5) - 240 فولت"]