{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AZQS-BV1"]
[]
[]
[]
[]
["","","","","","AZQS100B7V1B","AZQS125B7V1B","AZQS140B7V1B"]
["الأبعاد","الوحدة","","الارتفاع","mm","990","990","1430"]
["","","","العرض","mm","940","940","940"]
["","","","العمق","mm","320","320","320"]
["الوزن","الوحدة","","","kg","81","81","102"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-5","-5","-5"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","46","46","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-15","-15","-15"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","15.5","15.5","15.5"]
["مستوى طاقة الصوت","التبريد","","","dBA","70","71","70"]
["Sound pressure level","Cooling","","Nom.","dBA","53","54","53"]
["","Heating","","Nom.","dBA","57","58","54"]
["","Night quiet mode","","Level 1","dBA","49","49","49"]
["سائل تبريد","السعة","","","kg","2.9","2.9","4.0"]
["","GWP","","","","2087.5","2087.5","2087.5"]
["","السعة","","","tCO2Eq","6.1","6.1","8.4"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","15.9","15.9","15.9"]
["","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","50","50","50"]
["","","نظام","مكافئ","م","70","70","70"]
["","","","بدون شحن","م","30","30","30"]
["Piping connections","Level difference","IU - OU","Max.","م","30.0","30.0","30.0"]
["","","IU - IU","Max.","م","0.5","0.5","0.5"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["Power supply","Frequency","","","Hz","50","50","50"]