{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-BT"]
[]
[]
[]
[]
["","","","","","CTXA15B2V1BT"]
["Sound pressure level","Heating","","High","dBA","39"]
["","","","متوسط","dBA","32"]
["","","","Silent operation","dBA","21"]
["","","","Low","dBA","25"]
["","Cooling","","متوسط","dBA","32"]
["","","","Silent operation","dBA","21"]
["","","","Low","dBA","25"]
["","","","High","dBA","39"]
["Standard Accessories","دليل التركيب","","","","1"]
["","دليل التشغيل","","","","1"]
["","مرشح هواء","","","","2"]
["","جهاز تحكم عن بعد بالأشعة تحت الحمراء","","","","1"]
["","لوحة تثبيت جهاز التحكم عن بعد","","","","1"]
["","حقيبة المسامير اللولبية","","","","1"]
["","غطاء البراغي","","","","2"]
["","بطاريات جافة قياس AAA","","","","2"]
["","تدابير السلامة الوقائية العامة","","","","1"]
["Refrigerant","GWP","","","","675.0"]
["أنظمة التحكم","Wired remote control","","","","BRC073"]
["","Infrared remote control","","","","ARC466A58"]
["Piping connections","Liquid","","القطر الخارجي","mm","6.35"]
["","غاز","","القطر الخارجي","mm","9.50"]
["","Drain","","","","18"]
["Power input","Cooling","","Nom.","kW","0.020"]
["","Heating","","Nom.","kW","0.020"]
["Sound power level","التبريد","","","dBA","57"]
["Dimensions","Unit","","العرض","mm","798"]
["","","","العمق","mm","189"]
["","","","الارتفاع","mm","295"]
["الغلاف","اللون","","","","خشب أسود"]
["الوزن","الوحدة","","","kg","11.5"]
["Fan","Air flow rate","Heating","High","m³/min","10.9"]
["","","","متوسط","m³/min","8.7"]
["","","","Low","m³/min","6.4"]
["","","","Silent operation","m³/min","4.5"]
["","","Cooling","Low","m³/min","6.1"]
["","","","متوسط","m³/min","8.2"]
["","","","High","m³/min","11.0"]
["","","","Silent operation","m³/min","4.6"]
["Power supply","الطور","","","","1~"]
["","الاسم","","","","V1"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]