{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-A"]
[]
[]
[]
[]
["","","","","","CTXM15A2V1B","CTXM15A5V1B"]
["Power input","Cooling","","Nom.","kW","0.019","0.019"]
["","Heating","","Nom.","kW","0.018","0.018"]
["الغلاف","اللون","","","","أبيض","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","298","298"]
["","","","العرض","mm","804","804"]
["","","","العمق","mm","252","252"]
["الوزن","الوحدة","","","kg","11.5","11.5"]
["Fan","Air flow rate","Cooling","High","m³/min","11.9","11.9"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","8.9","8.9"]
["Fan","Air flow rate","Cooling","Low","m³/min","6.3","6.3"]
["","","","Silent operation","m³/min","4.9","4.9"]
["","","Heating","High","m³/min","11.4","11.4"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","9.2","9.2"]
["Fan","Air flow rate","Heating","Low","m³/min","6.9","6.9"]
["","","","Silent operation","m³/min","4.9","4.9"]
["مستوى طاقة الصوت","التبريد","","","dBA","54","54"]
["","التدفئة","","","dBA","53","53"]
["Sound pressure level","Cooling","","High","dBA","41","41"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","33","33"]
["Sound pressure level","Cooling","","Low","dBA","25","25"]
["","","","Silent operation","dBA","19","19"]
["","Heating","","High","dBA","39","39"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","34","34"]
["Sound pressure level","Heating","","Low","dBA","26","26"]
["","","","Silent operation","dBA","20","20"]
["سائل تبريد","GWP","","","","675","675"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.4","6.4"]
["","غاز","","القطر الخارجي","mm","9.5","9.5"]
["","التصريف","","","","16","16"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","ARC466A86","ARC466A86"]
["","جهاز تحكم عن بُعد سلكي","","","","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Installation plate","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["نطاق كفاءة استخدام الطاقة","","","","","A+++ ~ D","A+++ ~ D"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1"]
["","الطور","","","","1~","1~"]
["Power supply","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - التبريد: درجة الحرارة الداخلية 27 درجة مئوية للبويصلة الجافة، 19 درجة مئوية للبويصلة الرطبة؛ درجة الحرارة الخارجية: 35 درجة مئوية للبويصلة الجافة؛ الطول المكافئ للمواسير: 5 متر؛ فرق المستوى: 0 متر","(1) - التبريد: درجة الحرارة الداخلية 27 درجة مئوية للبويصلة الجافة، 19 درجة مئوية للبويصلة الرطبة؛ درجة الحرارة الخارجية: 35 درجة مئوية للبويصلة الجافة؛ الطول المكافئ للمواسير: 5 متر؛ فرق المستوى: 0 متر"]
["","","","","","(2) - التدفئة: درجة الحرارة الداخلية 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة؛ الطول المكافئ للمواسير: 5 متر؛ فرق المستوى: 0 متر","(2) - التدفئة: درجة الحرارة الداخلية 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة؛ الطول المكافئ للمواسير: 5 متر؛ فرق المستوى: 0 متر"]