{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R"]
[]
[]
[]
[]
["","","","","","CTXM15R2V1B","CTXM15R5V1B"]
["Power input","Cooling","","Nom.","kW","0.029","0.029"]
["","Heating","","Nom.","kW","0.023","0.023"]
["الغلاف","اللون","","","","أبيض","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","295","295"]
["","","","العرض","mm","778","778"]
["","","","العمق","mm","272","272"]
["الوزن","الوحدة","","","kg","10","10"]
["Fan","Air flow rate","Cooling","High","m³/min","10.5","10.5"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","7.5","7.5"]
["Fan","Air flow rate","Cooling","Low","m³/min","5.7","5.7"]
["","","","Silent operation","m³/min","4.3","4.3"]
["","","Heating","High","m³/min","9.3","9.3"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","8.2","8.2"]
["Fan","Air flow rate","Heating","Low","m³/min","6.2","6.2"]
["","","","Silent operation","m³/min","5.1","5.1"]
["مستوى طاقة الصوت","التبريد","","","dBA","57","57"]
["","التدفئة","","","dBA","54","54"]
["Sound pressure level","Cooling","","High","dBA","41","41"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","33","33"]
["Sound pressure level","Cooling","","Low","dBA","25","25"]
["","","","Silent operation","dBA","19","19"]
["","Heating","","High","dBA","39","39"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","34","34"]
["Sound pressure level","Heating","","Low","dBA","26","26"]
["","","","Silent operation","dBA","20","20"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.5","9.5"]
["","التصريف","","","","18","18"]
["أنظمة التحكم","Infrared remote control","","","","ARC466A67","ARC466A67"]
["أنظمة التحكم","جهاز تحكم عن بُعد سلكي","","","","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","WLAN adapter kit","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1"]
["","الطور","","","","1~","1~"]
["Power supply","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]