{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":57,"n_cols":9,"rows_kept":57,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","6.3","","7.2"]
["Sound pressure level","Cooling","","Nom.","dBA","31","","35"]
["Fan","Air flow rate","Heating","Nom.","m³/min","7.5","","8.1"]
["Sound pressure level","Heating","","Nom.","dBA","33"]
["Power input","Cooling","","Nom.","kW","0.04","0.04","0.040","0.040"]
["","Heating","","Nom.","kW","0.04","0.04","0.040","0.040"]
["الغلاف","اللون","","","","أبيض","أبيض","أبيض","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","289","289","289","289"]
["","","","العرض","mm","780","780","780","780"]
["","","","العمق","mm","215","215","215","215"]
["الوزن","الوحدة","","","kg","8","8","8","8.00"]
["Fan","Air flow rate","Cooling","High","m³/min","7.9","7.9","9.2","9.2"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","","6.3","","7.2"]
["Fan","Air flow rate","Cooling","Low","m³/min","4.7","4.7","5.2","5.2"]
["","","","Silent operation","m³/min","3.9","3.9","3.9","3.9"]
["","","Heating","High","m³/min","9","9","10.1","10.1"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","","7.5","","8.1"]
["Fan","Air flow rate","Heating","Low","m³/min","6","6","6.3","6.3"]
["","","","Silent operation","m³/min","4.3","4.3","4.3","4.3"]
["مستوى طاقة الصوت","التبريد","","","dBA","55","55","59","59"]
["","التدفئة","","","dBA","56","56","58","58"]
["Sound pressure level","Cooling","","High","dBA","37","37","42","42"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","","31","","35"]
["Sound pressure level","Cooling","","Low","dBA","25","25","28","28"]
["","","","Silent operation","dBA","21","21","21","21"]
["","Heating","","High","dBA","38","38","41","41"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","","33","","36"]
["Sound pressure level","Heating","","Low","dBA","28","28","30","30"]
["","","","Silent operation","dBA","21","21","21","21"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.5","9.5","9.5","9.50"]
["","التصريف","","","","18","18","18","18"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A6"]
["Standard Accessories","دليل التركيب","","","","1","1","1","1"]
["","جهاز تحكم عن بعد لاسلكي","","","","1","1","1","1"]
["","دليل التشغيل","","","","1","1","1","1"]
["","البطاريات","","","","2","","2"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","","2","2","2","2"]
["","لوح التثبيت","","","","1","1","1","1"]
["","حامل جهاز التحكم عن بعد","","","","1","1","1","1"]
["","مرشح تنقية الهواء بالتحفيز الضوئي وأباتيت التيتانيوم","","","","2","","2"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1","V1","V1"]
["","الطور","","","","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت"]
["","","","","","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت"]
["","","","","","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت"]
["Standard Accessories","بطاريات جافة قياس AAA","","","","","2","","2"]
["","مرشح أباتيت التيتانيوم المزيل للروائح","","","","","2","","2"]
["Notes","","","","","","(4) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها.","","(4) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها."]