{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Sound pressure level","Heating","","High","dBA","38","","41"]
["","","","Silent operation","dBA","21","","21"]
["","","","Low","dBA","28","","30"]
["","Cooling","","Silent operation","dBA","21","","21"]
["","","","Low","dBA","25","","28"]
["","","","High","dBA","37","","42"]
["","","","Nom.","dBA","33"]
["","Cooling","","Nom.","dBA","31","","35"]
["Standard Accessories","دليل التركيب","","","","1","","1"]
["","دليل التشغيل","","","","1","","1"]
["","جهاز تحكم عن بعد لاسلكي","","","","1","","1"]
["","البطاريات","","","","2","","2"]
["","حامل جهاز التحكم عن بعد","","","","1","","1"]
["","لوح التثبيت","","","","1","","1"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","","2","","2"]
["","مرشح تنقية الهواء بالتحفيز الضوئي وأباتيت التيتانيوم","","","","2","","2"]
["أنظمة التحكم","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Piping connections","Liquid","","القطر الخارجي","mm","6.35","","6.35"]
["","غاز","","القطر الخارجي","mm","9.5","","9.5"]
["","Drain","","","","18","","18"]
["Power input","Cooling","","Nom.","kW","0.040","","0.040"]
["","Heating","","Nom.","kW","0.040","","0.040"]
["Sound power level","التبريد","","","dBA","55","","59"]
["","التدفئة","","","dBA","56","","58"]
["Dimensions","Unit","","العرض","mm","780","","780"]
["","","","العمق","mm","215","","215"]
["","","","الارتفاع","mm","289","","289"]
["الغلاف","اللون","","","","White","","White"]
["الوزن","الوحدة","","","kg","8","","8"]
["Fan","Air flow rate","Heating","High","m³/min","","","10.1"]
["","","","Low","m³/min","","","6.3"]
["","","","Silent operation","m³/min","","","4.3"]
["","","Cooling","Low","m³/min","","","5.2"]
["","","","High","m³/min","","","9.2"]
["","","","Silent operation","m³/min","","","3.9"]
["","","","Nom.","m³/min","","","8.1"]
["","","Cooling","Nom.","m³/min","","","7.2"]
["Power supply","الطور","","","","1~","","1~"]
["","Frequency","","","Hz","50","","50"]
["","الاسم","","","","V1","","V1"]
["","Voltage","","","V","220-240","","220-240"]
["Notes","","","","","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت"]
["","","","","","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت"]
["","","","","","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت"]
["Power input","Cooling","","Nom.","kW","","0.04","","0.040"]
["","Heating","","Nom.","kW","","0.04","","0.040"]
["الغلاف","اللون","","","","","أبيض","","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","","289","","289"]
["","","","العرض","mm","","780","","780"]
["","","","العمق","mm","","215","","215"]
["الوزن","الوحدة","","","kg","","8","","8.00"]
["Fan","Air flow rate","Cooling","High","m³/min","","7.9","","9.2"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","","6.3","","7.2"]
["Fan","Air flow rate","Cooling","Low","m³/min","","4.7","","5.2"]
["","","","Silent operation","m³/min","","3.9","","3.9"]
["","","Heating","High","m³/min","","9","","10.1"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","","7.5","","8.1"]
["Fan","Air flow rate","Heating","Low","m³/min","","6","","6.3"]
["","","","Silent operation","m³/min","","4.3","","4.3"]
["مستوى طاقة الصوت","التبريد","","","dBA","","55","","59"]
["","التدفئة","","","dBA","","56","","58"]
["Sound pressure level","Cooling","","High","dBA","","37","","42"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","","31","","35"]
["Sound pressure level","Cooling","","Low","dBA","","25","","28"]
["","","","Silent operation","dBA","","21","","21"]
["","Heating","","High","dBA","","38","","41"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","","33","","36"]
["Sound pressure level","Heating","","Low","dBA","","28","","30"]
["","","","Silent operation","dBA","","21","","21"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","","6.35","","6.35"]
["","غاز","","القطر الخارجي","mm","","9.5","","9.50"]
["","التصريف","","","","","18","","18"]
["أنظمة التحكم","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Standard Accessories","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["وحدة التزويد بالطاقة","الاسم","","","","","V1","","V1"]
["","الطور","","","","","1~","","1~"]
["Power supply","Frequency","","","Hz","","50","","50"]
["","Voltage","","","V","","220-240","","220-240"]