{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":92,"n_cols":7,"rows_kept":92,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CVXM-A"]
[]
[]
[]
[]
["","","","","","CVXM20A2V1B","CVXM20A3V1B"]
["Sound pressure level","Heating","","High","dBA","38.0"]
["","","","متوسط","dBA","32.0"]
["","","","Silent operation","dBA","21.0"]
["","","","Low","dBA","25.0"]
["","Cooling","","متوسط","dBA","32.0"]
["","","","Silent operation","dBA","22.0"]
["","","","Low","dBA","25.0"]
["","","","High","dBA","38.0"]
["Standard Accessories","دليل التركيب","","","","1"]
["","دليل التشغيل","","","","1"]
["","جهاز تحكم عن بعد لاسلكي","","","","1"]
["","بطاريات جافة قياس AAA","","","","1"]
["","حامل جهاز التحكم عن بعد","","","","1"]
["","مرشح أباتيت التيتانيوم المزيل للروائح","","","","2"]
["","حقيبة المسامير اللولبية","","","","1"]
["","تدابير السلامة الوقائية العامة","","","","1"]
["Refrigerant","GWP","","","","675.0"]
["أنظمة التحكم","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A66"]
["Piping connections","Liquid","","القطر الخارجي","mm","6.35"]
["","غاز","","القطر الخارجي","mm","9.50"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)"]
["Power input","Cooling","","Nom.","kW","0.02"]
["","Heating","","Nom.","kW","0.02"]
["Sound power level","التبريد","","","dBA","52.0"]
["","التدفئة","","","dBA","52.0"]
["Dimensions","Unit","","العرض","mm","750"]
["","","","العمق","mm","238"]
["","","","الارتفاع","mm","600"]
["الغلاف","اللون","","","","White"]
["الوزن","الوحدة","","","kg","17"]
["Fan","Air flow rate","Heating","High","m³/min","9.2"]
["","","","Low","m³/min","5.6"]
["","","","متوسط","m³/min","7.2"]
["","","","Silent operation","m³/min","4.1"]
["","","Cooling","Low","m³/min","4.9"]
["","","","متوسط","m³/min","7"]
["","","","High","m³/min","8.7"]
["","","","Silent operation","m³/min","4.1"]
["Power supply","الطور","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - التبريد: درجة الحرارة الداخلية 27 درجة مئوية للبويصلة الجافة، 19.0 درجة مئوية للبويصلة الرطبة؛ درجة الحرارة الخارجية 35 درجة مئوية للبويصلة الجافة، 24 درجة مئوية للبويصلة الرطبة؛ الطول المكافئ للمواسير: 5 متر"]
["","","","","","(2) - التدفئة: درجة الحرارة الداخلية 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة؛ الطول المكافئ للمواسير: 5 متر"]
["Power input","Cooling","","Nom.","kW","","0.02"]
["","Heating","","Nom.","kW","","0.02"]
["الغلاف","اللون","","","","","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","","600"]
["","","","العرض","mm","","750"]
["","","","العمق","mm","","238"]
["الوزن","الوحدة","","","kg","","17"]
["Fan","Air flow rate","Cooling","High","m³/min","","8.7"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","","7"]
["Fan","Air flow rate","Cooling","Low","m³/min","","4.9"]
["","","","Silent operation","m³/min","","4.1"]
["","","Heating","High","m³/min","","9.2"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","","7.2"]
["Fan","Air flow rate","Heating","Low","m³/min","","5.6"]
["","","","Silent operation","m³/min","","4.1"]
["مستوى طاقة الصوت","التبريد","","","dBA","","52"]
["","التدفئة","","","dBA","","52"]
["Sound pressure level","Cooling","","High","dBA","","38"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","","32"]
["Sound pressure level","Cooling","","Low","dBA","","25"]
["","","","Silent operation","dBA","","22"]
["","Heating","","High","dBA","","38"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","","32"]
["Sound pressure level","Heating","","Low","dBA","","25"]
["","","","Silent operation","dBA","","21"]
["سائل تبريد","GWP","","","","","675"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","","6.4"]
["","غاز","","القطر الخارجي","mm","","9.5"]
["","التصريف","","","","","VP20 (I.D. 20/O.D. 26)"]
["أنظمة التحكم","Infrared remote control","","","","","ARC466A66"]
["أنظمة التحكم","جهاز تحكم عن بُعد سلكي","","","","","BRC073A1"]
["Standard Accessories","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","1"]
["","General safety precautions","","","","","1"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Remote control holder","","","","","1"]
["","Screw bag","","","","","1"]
["وحدة التزويد بالطاقة","الطور","","","","","1~"]
["Power supply","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]