{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCM010A51"]
[]
[]
[]
[]
["","","","","DCM010A51."]
["وحدة قابلة للتوصيل","","","","داخلي ، خارجي، صندوق مائي، أنواع تهوية من نقاط إدارة iTM"]
["الدخل","الكمبيوتر","البرنامج","","Microsoft Windows 7، و8، و8.1، و10, Microsoft Server 2012 و2016"]
["Maximum number of connectable indoor units","","","","2,500 (2)"]
["الحد الأعلى لعدد الوحدات الخارجية القابلة للتوصيل","","","","400 (3)"]
["Notes","","","","(1) - متوافق مع إصدارات Oracle PMS: Opera v5.0.03.03 e43، وv5.0.04.01 e24، وv5.0.04.02 e17، وv5.0.04.02 e17، وv5.0.04.03 e10، وv5.0.05.00 وأعلى"]
["","","","","(2) - وحدات داخلية 5 × 500 لكل جهاز تحكم iTM"]
["","","","","(3) - أنظمة خارجية 5 × 80 لكل جهاز تحكم iTM"]
["","","","","(4) - تنزيل البرنامج مجاناً، مفتاح ترخيص بتنسيق فعلي (ورق)"]
["","","","","(5) - مطلوب ترخيص واحد DCM010A51 وDCM007A51 لكل جهاز تحكم iTM"]