{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":7,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBH-CB3VU / ERLQ-CV3"]
[]
[]
[]
[]
["","","","","EHBH04CB3VU / ERLQ004CAV3","EHBH08CB3VU / ERLQ006CAV3","EHBH08CB3VU / ERLQ008CAV3"]
["COP","","","","5.04 (1), 3.58 (2)","4.74 (1), 3.56 (2)","5.04 (1), 3.58 (2)"]
["Heating capacity","Nom.","","kW","4.40 (1), 4.03 (2)","6.00 (1), 5.67 (2)","4.40 (1), 4.03 (2)"]
["","Min.","","kW","1.80 (1)","1.80 (1)","1.80 (1)"]
["","Max.","","kW","5.12 (1), 4.90 (2)","8.35 (1), 7.95 (2)","5.12 (1), 4.90 (2)"]
["Power input","Heating","Nom.","kW","0.870 (1), 1.13 (2)","1.27 (1), 1.59 (2)","0.870 (1), 1.13 (2)"]
["Notes","","","","(1) - الحالة 1: التبريد Ta‏ 35‏° مئوية  - LWE‏ 18‏° مئوية (DT‏ = 5‏° مئوية)؛ التدفئة Ta الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 35‏° مئوية (DT‏ = 5‏° مئوية)","(1) - الحالة 1: التبريد Ta‏ 35‏° مئوية  - LWE‏ 18‏° مئوية (DT‏ = 5‏° مئوية)؛ التدفئة Ta الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 35‏° مئوية (DT‏ = 5‏° مئوية)","(1) - الحالة 1: التبريد Ta‏ 35‏° مئوية  - LWE‏ 18‏° مئوية (DT‏ = 5‏° مئوية)؛ التدفئة Ta الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 35‏° مئوية (DT‏ = 5‏° مئوية)"]
["","","","","(2) - الحالة 2: التبريد Ta‏ 35‏° مئوية  - LWE‏ 7‏° مئوية (DT‏ = 5‏° مئوية)؛ التدفئة Ta الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (DT‏ = 5‏° مئوية)","(2) - الحالة 2: التبريد Ta‏ 35‏° مئوية  - LWE‏ 7‏° مئوية (DT‏ = 5‏° مئوية)؛ التدفئة Ta الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (DT‏ = 5‏° مئوية)","(2) - الحالة 2: التبريد Ta‏ 35‏° مئوية  - LWE‏ 7‏° مئوية (DT‏ = 5‏° مئوية)؛ التدفئة Ta الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (DT‏ = 5‏° مئوية)"]
["","","","","(3) - Tamb‏ 35‏° مئوية - LWE‏ 7‏° مئوية (DT‏=5‏°مئوية)","(3) - Tamb‏ 35‏° مئوية - LWE‏ 7‏° مئوية (DT‏=5‏°مئوية)","(3) - Tamb‏ 35‏° مئوية - LWE‏ 7‏° مئوية (DT‏=5‏°مئوية)"]
["","","","","(4) - Tamb‏ 35‏° مئوية - LWE‏ 18‏° مئوية (DT‏=5‏°مئوية)","(4) - Tamb‏ 35‏° مئوية - LWE‏ 18‏° مئوية (DT‏=5‏°مئوية)","(4) - Tamb‏ 35‏° مئوية - LWE‏ 18‏° مئوية (DT‏=5‏°مئوية)"]
["","","","","(5) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(5) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(5) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)"]
["","","","","(6) - الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (Dt‏=5‏° مئوية)","(6) - الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (Dt‏=5‏° مئوية)","(6) - الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (Dt‏=5‏° مئوية)"]