{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":10,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBX-C / ERHQ-BV3"]
[]
[]
[]
[]
["","","","","EHBX16CA3V / ERHQ011BAV3","EHBX16CA9W / ERHQ011BAV3","EHBX16CA3V / ERHQ014BAV3","EHBX16CA9W / ERHQ014BAV3","EHBX16CA3V / ERHQ016BAV3","EHBX16CA9W / ERHQ016BAV3"]
["COP","","","","4.39 (3), 3.25 (4)","4.39 (3), 3.25 (4)","4.29 (3), 3.24 (4)","4.29 (3), 3.24 (4)","4.08 (3), 3.20 (4)","4.08 (3), 3.20 (4)"]
["Cooling capacity","Nom.","","kW","13.9 (2), 10.0 (1)","13.9 (2), 10.0 (1)","17.3 (2), 12.5 (1)","17.3 (2), 12.5 (1)","17.8 (2), 13.1 (1)","17.8 (2), 13.1 (1)"]
["EER","","","","3.60 (2), 2.71 (1)","3.60 (2), 2.71 (1)","2.95 (2), 2.32 (1)","2.95 (2), 2.32 (1)","2.59 (2), 2.20 (1)","2.59 (2), 2.20 (1)"]
["Heating capacity","Nom.","","kW","11.2 (3), 10.30 (4)","11.2 (3), 10.30 (4)","14.0 (3), 13.1 (4)","14.0 (3), 13.1 (4)","16.0 (3), 15.2 (4)","16.0 (3), 15.2 (4)"]
["Power input","Cooling","Nom.","kW","3.86 (2), 3.69 (1)","3.86 (2), 3.69 (1)","5.86 (2), 5.39 (1)","5.86 (2), 5.39 (1)","6.87 (2), 5.95 (1)","6.87 (2), 5.95 (1)"]
["","Heating","Nom.","kW","2.55 (3), 3.17 (4)","2.55 (3), 3.17 (4)","3.26 (3), 4.04 (4)","3.26 (3), 4.04 (4)","3.92 (3), 4.75 (4)","3.92 (3), 4.75 (4)"]
["Notes","","","","(1) - Tamb‏ 35‏° مئوية - LWE‏ 7‏° مئوية (DT‏=5‏°مئوية)","(1) - Tamb‏ 35‏° مئوية - LWE‏ 7‏° مئوية (DT‏=5‏°مئوية)","(1) - Tamb‏ 35‏° مئوية - LWE‏ 7‏° مئوية (DT‏=5‏°مئوية)","(1) - Tamb‏ 35‏° مئوية - LWE‏ 7‏° مئوية (DT‏=5‏°مئوية)","(1) - Tamb‏ 35‏° مئوية - LWE‏ 7‏° مئوية (DT‏=5‏°مئوية)","(1) - Tamb‏ 35‏° مئوية - LWE‏ 7‏° مئوية (DT‏=5‏°مئوية)"]
["","","","","(2) - Tamb‏ 35‏° مئوية - LWE‏ 18‏° مئوية (DT‏=5‏°مئوية)","(2) - Tamb‏ 35‏° مئوية - LWE‏ 18‏° مئوية (DT‏=5‏°مئوية)","(2) - Tamb‏ 35‏° مئوية - LWE‏ 18‏° مئوية (DT‏=5‏°مئوية)","(2) - Tamb‏ 35‏° مئوية - LWE‏ 18‏° مئوية (DT‏=5‏°مئوية)","(2) - Tamb‏ 35‏° مئوية - LWE‏ 18‏° مئوية (DT‏=5‏°مئوية)","(2) - Tamb‏ 35‏° مئوية - LWE‏ 18‏° مئوية (DT‏=5‏°مئوية)"]
["","","","","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)"]
["","","","","(4) - الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (Dt‏=5‏° مئوية)","(4) - الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (Dt‏=5‏° مئوية)","(4) - الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (Dt‏=5‏° مئوية)","(4) - الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (Dt‏=5‏° مئوية)","(4) - الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (Dt‏=5‏° مئوية)","(4) - الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (Dt‏=5‏° مئوية)"]