{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":8,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVZ-CB3V / ERHQ-BV3"]
[]
[]
[]
[]
["","","","","","EHVZ16S18CB3V / ERHQ011BAV3","EHVZ16S18CB3V / ERHQ014BAV3","EHVZ16S18CB3V / ERHQ016BAV3"]
["Heating capacity","Nom.","","","kW","11.2, 10.3","14.0, 13.1","16.0, 15.2"]
["Power input","Heating","","Nom.","kW","2.55, 3.17","3.26, 4.04","3.92, 4.75"]
["COP","","","","","4.39, 3.25","4.29, 3.24","4.08, 3.20"]
["تسخين الماء المنزلي","عام","","ملف تعريف الحمل المعلن عنه","","L","L","L"]
["","المناخ المعتدل","","فئة فعالية طاقة تسخين الماء","","A","A","A"]
["تدفئة المساحة","معدل مخرج الماء المناخي 55°مئوية","عام","SCOP","","2.86","2.82","2.92"]
["","","","فئة فعالية مساحة التدفئة الفصلية","","A+","A+","A+"]
["","معدل مخرج الماء المناخي 35°مئوية","عام","SCOP","","2.99","3.23","3.29"]
["","","","فئة فعالية مساحة التدفئة الفصلية","","A++","A+","A+"]
["نطاق كفاءة استخدام الطاقة","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Notes","","","","","(1) - الحالة 1: التبريد Ta‏ 35‏° مئوية  - LWE‏ 18‏° مئوية (DT‏ = 5‏° مئوية)؛ التدفئة Ta الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 35‏° مئوية (DT‏ = 5‏° مئوية)","(1) - الحالة 1: التبريد Ta‏ 35‏° مئوية  - LWE‏ 18‏° مئوية (DT‏ = 5‏° مئوية)؛ التدفئة Ta الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 35‏° مئوية (DT‏ = 5‏° مئوية)","(1) - الحالة 1: التبريد Ta‏ 35‏° مئوية  - LWE‏ 18‏° مئوية (DT‏ = 5‏° مئوية)؛ التدفئة Ta الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 35‏° مئوية (DT‏ = 5‏° مئوية)"]
["","","","","","(2) - الحالة 2: التبريد Ta‏ 35‏° مئوية  - LWE‏ 7‏° مئوية (DT‏ = 5‏° مئوية)؛ التدفئة Ta الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (DT‏ = 5‏° مئوية)","(2) - الحالة 2: التبريد Ta‏ 35‏° مئوية  - LWE‏ 7‏° مئوية (DT‏ = 5‏° مئوية)؛ التدفئة Ta الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (DT‏ = 5‏° مئوية)","(2) - الحالة 2: التبريد Ta‏ 35‏° مئوية  - LWE‏ 7‏° مئوية (DT‏ = 5‏° مئوية)؛ التدفئة Ta الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (DT‏ = 5‏° مئوية)"]
["","","","","","","(3) - يجب تجزئة الاستطاعة بين المنطقة الأساسية والإضافية. راجع بيانات الضغط الاستاتيكي الخارجي ESP للحصول على مزيد من التفاصيل حول الرأس المتوفر (كيلو باسكال).","(3) - يجب تجزئة الاستطاعة بين المنطقة الأساسية والإضافية. راجع بيانات الضغط الاستاتيكي الخارجي ESP للحصول على مزيد من التفاصيل حول الرأس المتوفر (كيلو باسكال)."]