{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERHQ-BBV3"]
[]
[]
[]
[]
["","","","","","ERHQ006BBV3","ERHQ007BBV3","ERHQ008BBV3"]
["Sound pressure level","Heating","","Nom.","dBA","48","48","49"]
["","Cooling","","Nom.","dBA","48","48","50"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["Sound power level","Heating","","Nom.","dBA","61","61","62"]
["","Cooling","","Nom.","dBA","63","63","63"]
["Refrigerant","Charge","","","TCO2Eq","3.5","3.5","3.5"]
["","GWP","","","","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","1.7","1.7","1.7"]
["","النوع","","","","R-410A","R-410A","R-410A"]
["Dimensions","Unit","","العرض","mm","825","825","825"]
["","","","العمق","mm","300","300","300"]
["","","","الارتفاع","mm","735","735","735"]
["الوزن","الوحدة","","","kg","56","56","56"]
["Piping connections","Liquid","","القطر الخارجي","mm","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","15.9","15.9","15.9"]
["","Drain","","OD","mm","20","20","20"]
["","Level difference","IU - OU","Max.","م","20","20","20"]
["Power supply","الطور","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","الاسم","","","","V3","V3","V3"]
["","Voltage","","","V","230","230","230"]
["Current","الفواصم المنصوح بها","","","A","20","20","20"]
["Notes","","","","","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","(2) - نطاق التشغيل للتسخين (الوحدة الخارجية): يتزايد النطاق بالدعم الذي يوفره السخان الاحتياطي","(2) - نطاق التشغيل للتسخين (الوحدة الخارجية): يتزايد النطاق بالدعم الذي يوفره السخان الاحتياطي","(2) - نطاق التشغيل للتسخين (الوحدة الخارجية): يتزايد النطاق بالدعم الذي يوفره السخان الاحتياطي"]
["","","","","","(3) - نطاق التشغيل للماء الساخن المنزلي (الوحدة الخارجية): يتزايد النطاق بالدعم الذي يوفره السخان المعزز","(3) - نطاق التشغيل للماء الساخن المنزلي (الوحدة الخارجية): يتزايد النطاق بالدعم الذي يوفره السخان المعزز","(3) - نطاق التشغيل للماء الساخن المنزلي (الوحدة الخارجية): يتزايد النطاق بالدعم الذي يوفره السخان المعزز"]
["","","","","","(4) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(4) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(4) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information."]
["","","","","","(5) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","(5) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","(5) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase"]
["","","","","","(6) - بالتوافق مع EN/IEC 61000-3-11‎‏، قد يكون من الضوري استشارة مشغل شبكة التوزيع للتأكد من أن الجهاز موصول بتغذية ممانعتها Zsys (ممانعة النظام) ≤ Zmax","(6) - بالتوافق مع EN/IEC 61000-3-11‎‏، قد يكون من الضوري استشارة مشغل شبكة التوزيع للتأكد من أن الجهاز موصول بتغذية ممانعتها Zsys (ممانعة النظام) ≤ Zmax","(6) - بالتوافق مع EN/IEC 61000-3-11‎‏، قد يكون من الضوري استشارة مشغل شبكة التوزيع للتأكد من أن الجهاز موصول بتغذية ممانعتها Zsys (ممانعة النظام) ≤ Zmax"]
["","","","","","(7) - EN/IEC 61000-3-11: European/international technical standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated ≤ 75A","(7) - EN/IEC 61000-3-11: European/international technical standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated ≤ 75A","(7) - EN/IEC 61000-3-11: European/international technical standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated ≤ 75A"]
["","","","","","(8) - فئة وحدة PED: مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC","(8) - فئة وحدة PED: مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC","(8) - فئة وحدة PED: مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC"]
["","","","","","(9) - يحتوي على غازات الاحتباس الحراري المفلورة","(9) - يحتوي على غازات الاحتباس الحراري المفلورة","(9) - يحتوي على غازات الاحتباس الحراري المفلورة"]