{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERLQ-BW1"]
[]
[]
[]
[]
["","","","","","ERLQ011BAW1","ERLQ014BAW1","ERLQ016BAW1"]
["Sound pressure level","Heating","","Nom.","dBA","51","51","52"]
["","Cooling","","Nom.","dBA","50","52","54"]
["Standard Accessories","أغلفة برباط","","","","2","2","2"]
["","Installation manual","","","","1","1","1"]
["Sound power level","Heating","","Nom.","dBA","64","64","66"]
["","Cooling","","Nom.","dBA","64","66","69"]
["Refrigerant","Charge","","","TCO2Eq","6.2","6.2","6.2"]
["","GWP","","","","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","2.95","2.95","2.95"]
["","النوع","","","","R-410A","R-410A","R-410A"]
["Dimensions","Unit","","العرض","mm","900","900","900"]
["","","","العمق","mm","320","320","320"]
["","","","الارتفاع","mm","1,345","1,345","1,345"]
["الوزن","الوحدة","","","kg","108","108","108"]
["Piping connections","العزل الحراري","","","","Both liquid and gas pipes","Both liquid and gas pipes","Both liquid and gas pipes"]
["","Liquid","","القطر الخارجي","mm","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","15.9","15.9","15.9"]
["","Drain","","OD","mm","26","26","26"]
["","Level difference","IU - OU","Max.","م","30","30","30"]
["Power supply","الطور","","","","3N~","3N~","3N~"]
["","Frequency","","","Hz","50","50","50"]
["","الاسم","","","","W1","W1","W1"]
["","Voltage","","","V","400","400","400"]
["Current","الفواصم المنصوح بها","","","A","20","20","20"]
["Notes","","","","","(1) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(1) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(1) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information."]
["","","","","","(2) - Down to 3m with recharging of the outdoor unit. Please refer to the installation manual of the outdoor unit.","(2) - Down to 3m with recharging of the outdoor unit. Please refer to the installation manual of the outdoor unit.","(2) - Down to 3m with recharging of the outdoor unit. Please refer to the installation manual of the outdoor unit."]
["","","","","","(3) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(4) - Cooling Ta 35°C - LWE 18°C (DT = 5°C); Heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(4) - Cooling Ta 35°C - LWE 18°C (DT = 5°C); Heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(4) - Cooling Ta 35°C - LWE 18°C (DT = 5°C); Heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(5) - يحتوي على غازات الاحتباس الحراري المفلورة","(5) - يحتوي على غازات الاحتباس الحراري المفلورة","(5) - يحتوي على غازات الاحتباس الحراري المفلورة"]