{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":7,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-A"]
[]
[]
[]
[]
["","","","","","FAA71AUVEB","FAA100AUVEB"]
["الغلاف","اللون","","","","أبيض صاف","أبيض صاف"]
["","المادة","","","","Resin","Resin"]
["الأبعاد","الوحدة","","الارتفاع","mm","290","340"]
["","","","العرض","mm","1050","1200"]
["","","","العمق","mm","238","240"]
["الوزن","الوحدة","","","kg","13.0","17.0"]
["Fan","Air flow rate","Cooling","High","m³/min","18.0","26.0"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","16","23"]
["Fan","Air flow rate","Cooling","Low","m³/min","14.0","19.0"]
["","","Heating","High","m³/min","18.0","26.0"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","16.0","23.0"]
["Fan","Air flow rate","Heating","Low","m³/min","14.0","19.0"]
["مستوى طاقة الصوت","التبريد","","","dBA","61","65"]
["","التدفئة","","","dBA","61","65"]
["Sound pressure level","Cooling","","High","dBA","45","49"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","42","45"]
["Sound pressure level","Cooling","","Low","dBA","40","41"]
["","Heating","","High","dBA","45","49"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","42","45"]
["Sound pressure level","Heating","","Low","dBA","40","41"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","15.9","15.9"]
["","التصريف","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["أنظمة التحكم","جهاز تحكم عن بُعد سلكي","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~"]
["Power supply","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]