{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":60,"n_cols":7,"rows_kept":60,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-A"]
[]
[]
[]
[]
["","","","","","FAA71AUVEB","FAA100AUVEB"]
["Sound pressure level","Heating","","High","dBA","45"]
["","","","متوسط","dBA","42"]
["","","","Low","dBA","40"]
["","Cooling","","متوسط","dBA","42"]
["","","","Low","dBA","40"]
["","","","High","dBA","45"]
["أنظمة التحكم","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Piping connections","Liquid","","القطر الخارجي","mm","9.52"]
["","غاز","","القطر الخارجي","mm","15.9"]
["","Drain","","","","VP13 (I.D. 13/O.D. 18)"]
["Sound power level","التبريد","","","dBA","61"]
["","التدفئة","","","dBA","61"]
["Dimensions","Unit","","العرض","mm","1,050"]
["","","","العمق","mm","238"]
["","","","الارتفاع","mm","290"]
["الغلاف","المادة","","","","Resin"]
["","اللون","","","","أبيض صاف"]
["الوزن","الوحدة","","","kg","13.0"]
["Fan","Air flow rate","Heating","High","m³/min","18.0"]
["","","","Low","m³/min","14.0"]
["","","","متوسط","m³/min","16.0"]
["","","Cooling","Low","m³/min","14.0"]
["","","","متوسط","m³/min","16"]
["","","","High","m³/min","18.0"]
["Power supply","الطور","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["الغلاف","اللون","","","","","أبيض صاف"]
["","المادة","","","","","Resin"]
["الأبعاد","الوحدة","","الارتفاع","mm","","340"]
["","","","العرض","mm","","1200"]
["","","","العمق","mm","","240"]
["الوزن","الوحدة","","","kg","","17.0"]
["Fan","Air flow rate","Cooling","High","m³/min","","26.0"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","","23"]
["Fan","Air flow rate","Cooling","Low","m³/min","","19.0"]
["","","Heating","High","m³/min","","26.0"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","","23.0"]
["Fan","Air flow rate","Heating","Low","m³/min","","19.0"]
["مستوى طاقة الصوت","التبريد","","","dBA","","65"]
["","التدفئة","","","dBA","","65"]
["Sound pressure level","Cooling","","High","dBA","","49"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","","45"]
["Sound pressure level","Cooling","","Low","dBA","","41"]
["","Heating","","High","dBA","","49"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","","45"]
["Sound pressure level","Heating","","Low","dBA","","41"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","","9.52"]
["","غاز","","القطر الخارجي","mm","","15.9"]
["","التصريف","","","","","VP13 (I.D. 13/O.D. 18)"]
["أنظمة التحكم","جهاز تحكم عن بُعد سلكي","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["وحدة التزويد بالطاقة","الطور","","","","","1~"]
["Power supply","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]