{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-B / RZQ-DV1"]
[]
[]
[]
[]
["","","","","FAQ71BVV1B / RZQ71D7V1B","FAQ100BVV1B / RZQ100D7V1B"]
["Cooling capacity","Nom.","","kW","7.1 (1)","10.0 (1)"]
["Piping connections","Liquid","القطر الخارجي","mm","9.52","9.52"]
["","غاز","القطر الخارجي","mm","15.9","15.9"]
["","Drain","OD","mm","26","26"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","1,141","1,645"]
["","نسبة فعالية استهلاك الطاقة","","","3.11","3.04"]
["","عامل الأداء","","","3.43","3.49"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","B","B"]
["","","تدفئة","","B","B"]
["Heating capacity","Nom.","","kW","8.0 (2)","11.2 (2)"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m"]
["","","","","(3) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(3) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]