{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-B"]
[]
[]
[]
[]
["","","","","","FAQ71BVV1B","FAQ100BVV1B"]
["الغلاف","اللون","","","","أبيض","أبيض"]
["","المادة","","","","Resin","Resin"]
["الأبعاد","الوحدة","","الارتفاع","mm","290","360"]
["","","","العرض","mm","1050","1570"]
["","","","العمق","mm","230","200"]
["الوزن","الوحدة","","","kg","13.0","26.0"]
["Fan","Air flow rate","Cooling","High","m³/min","19.0","23.0"]
["","","","Low","m³/min","15.0","19.0"]
["","","Heating","High","m³/min","19.0","23.0"]
["","","","Low","m³/min","15.0","19.0"]
["مستوى طاقة الصوت","التبريد","","","dBA","59.0","61.0"]
["","التدفئة","","","dBA","59.0","61.0"]
["Sound pressure level","Cooling","","High","dBA","43.0","45.0"]
["","","","Low","dBA","37.0","41.0"]
["","Heating","","High","dBA","43.0","45.0"]
["","","","Low","dBA","37.0","41.0"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","15.9","15.9"]
["","التصريف","","","","VP13 (I.D. 13/O.D. 18)","VP20 (I.D. 20/O.D. 26)"]
["Standard Accessories","دليل التركيب والتشغيل","","","","1","1"]
["","لوحة التركيب","","","","لوحة التركيب","لوحة التركيب"]
["","عازل لأدوات التثبيت","","","","","عازل لأدوات التثبيت"]
["","شريط عزل","","","","شريط عزل","شريط عزل"]
["","نموذج ورق للتركيب","","","","نموذج ورق للتركيب","نموذج ورق للتركيب"]
["","مسامير لولبية","","","","مسامير لولبية","مسامير لولبية"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~"]
["Power supply","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - يتم قياس مستوى ضغط الصوت عبر ميكروفون على مسافة 1 متر من الوحدة.","(1) - يتم قياس مستوى ضغط الصوت عبر ميكروفون على مسافة 1 متر من الوحدة."]
["","","","","","(2) - مستوى ضغط الصوت هو قيمة نسبية، تعتمد على المسافة والبيئة الصوتية. لمزيد من التفاصيل، يرجى الرجوع إلى مخططات مستوى الصوت.","(2) - مستوى ضغط الصوت هو قيمة نسبية، تعتمد على المسافة والبيئة الصوتية. لمزيد من التفاصيل، يرجى الرجوع إلى مخططات مستوى الصوت."]
["","","","","","(3) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(3) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت."]