{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C / RZQSG-L(3/8)V1"]
[]
[]
[]
[]
["","","","","FAQ100CVEB / RZQSG100L8V1B"]
["Cooling capacity","Nom.","","kW","9.5"]
["تبريد المساحة","SEER","","","5.61"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","592.692"]
["","الاستطاعة","Pdesign","kW","9.50"]
["","فئة فعالية استهلاك الطاقة","","","A+"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","6.81"]
["","SCOP/A","","","4.01"]
["","فئة فعالية استهلاك الطاقة","","","A+"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","2,377.556"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","1,580"]
["","نسبة فعالية استهلاك الطاقة","","","3.01"]
["","عامل الأداء","","","3.41"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","B"]
["","","تدفئة","","B"]
["Heating capacity","Nom.","","kW","10.8"]
["Notes","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]