{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":4,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / RZQG-LV1L"]
[]
[]
[]
[]
["","","","FBA71A2VEB / RZQG71L9V1L"]
["Cooling capacity","Max.","kW","8.00 (1)"]
["","Nom.","kW","6.80 (1)"]
["الفعالية الاسمية","نسبة فعالية استهلاك الطاقة","","3.60 (1)"]
["","عامل الأداء","","4.01 (2)"]
["Heating capacity","Nom.","kW","7.50 (2)"]
["","Max.","kW","9.00 (2)"]
["Notes","","","(1) - التبريد: درجة الحرارة الداخلية 27 درجة مئوية للبويصلة الجافة، 19 درجة مئوية للبويصلة الرطبة، درجة الحرارة الخارجية 35 درجة مئوية للبويصلة الجافة"]
["","","","(2) - التدفئة: درجة الحرارة الداخلية 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة."]
["","","","(3) - عامل التحويل: 1كيلوواط=3412.14163 وحدة حرارية/سا (btu/hr)"]