{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A"]
[]
[]
[]
[]
["","","","","","FBA35A2VEB","FBA50A2VEB","FBA60A2VEB","FBA71A2VEB"]
["مروحة","الضغط الاستاتيكي الخارجي","","عالٍ","باسكال","150","150","150","150"]
["الغلاف","اللون","","","","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)"]
["","المادة","","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["الأبعاد","الوحدة","","الارتفاع","mm","245","245","245","245"]
["","","","العرض","mm","700","700","1000","1000"]
["","","","العمق","mm","800","800","800","800"]
["الوزن","الوحدة","","","kg","28","28","35","35"]
["Fan","Air flow rate","Cooling","High","m³/min","15","15","18","18"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","12.5","12.5","15","15"]
["Fan","Air flow rate","Cooling","Low","m³/min","10.5","10.5","12.5","12.5"]
["","","Heating","High","m³/min","15","15","18","18"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","12.5","12.5","15","15"]
["Fan","Air flow rate","Heating","Low","m³/min","10.5","10.5","12.5","12.5"]
["مروحة","الضغط الاستاتيكي الخارجي","","الإسمي","باسكال","30","30","30","30"]
["مستوى طاقة الصوت","التبريد","","","dBA","60","60","56","56"]
["Sound pressure level","Cooling","","High","dBA","35","35","30","30"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","32","32","28","28"]
["Sound pressure level","Cooling","","Low","dBA","29","29","25","25"]
["","Heating","","High","dBA","37","37","31","31"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","34","34","28","28"]
["Sound pressure level","Heating","","Low","dBA","29","29","25","25"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35","9.52"]
["","غاز","","القطر الخارجي","mm","9.52","12.7","12.7","15.9"]
["","التصريف","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["ارتفاع الصرف","mm","","","","625","625","625","625"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["","جهاز تحكم عن بُعد سلكي","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Standard Accessories","دليل التركيب","","","","1","1","1","1"]
["","حلقة للدعامة الحاملة","","","","8","8","8","8"]
["","دليل التشغيل","","","","1","1","1","1"]
["","مشابك","","","","4","4","4","4"]
["","خرطوم الصرف","","","","1","1","1","1"]
["","عازل لأدوات التثبيت","","","","2","2","2","2"]
["","مشبك معدني لخرطوم الصرف","","","","1","1","1","1"]
["","مسامير لولبية","","","","40","40","40","40"]
["","لباد مانع للتسريب","","","","5","5","5","5"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50/60","50/60","50/60","50/60"]
["","Voltage","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","","(1) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(1) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(1) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(1) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت."]
["","","","","","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]