{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":6,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C / RXS-G"]
[]
[]
[]
[]
["","","","","FBQ35C7VEB / RXS35G2V1B","FBQ50C7VEB / RXS50G2V1B"]
["Cooling capacity","Nom.","","kW","3.40 (1)","5.0 (1)"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","530","825"]
["","نسبة فعالية استهلاك الطاقة","","","3.21","3.03"]
["","عامل الأداء","","","3.51","3.42"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","B"]
["","","تدفئة","","B","B"]
["Heating capacity","Nom.","","kW","4.00 (2)","5.50 (2)"]
["Notes","","","","(1) - التبريد: درجة الحرارة الداخلية 27 درجة مئوية للبويصلة الجافة، 19.0 درجة مئوية للبويصلة الرطبة؛ درجة الحرارة الخارجية 35 درجة مئوية للبويصلة الجافة؛ الطول المكافئ للمواسير: 5 متر؛ فرق المستوى: 0 متر","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","(2) - التدفئة: درجة الحرارة الداخلية 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة؛ الطول المكافئ للمواسير: 5 متر؛ فرق المستوى: 0 متر","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m"]
["","","","","(3) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(3) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]