{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":11,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8"]
[]
[]
[]
[]
["","","","","FBQ35C8VEB","FBQ50C8VEB","FBQ60C8VEB","FBQ71C8VEB","FBQ100C8VEB","FBQ125C8VEB","FBQ140C8VEB"]
["Sound pressure level","Heating","High","dBA","37","37","37","37","38","40","41"]
["","","Low","dBA","29","29","29","29","32","33","34"]
["","Cooling","Low","dBA","29","29","29","29","32","33","33"]
["","","High","dBA","37","37","37","37","38","40","40"]
["Cooling capacity","Total capacity","Nom.","kW","3.4 (1)","5.0 (1)","5.7 (1)","7.1 (1)","10.0 (1)","12.5 (1)","13.4 (1)"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","غاز","القطر الخارجي","mm","9.5","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Drain","","","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)"]
["Power input","Cooling","Nom.","kW","0.140","0.140","0.350","0.350","0.350","0.350","0.350"]
["","Heating","Nom.","kW","0.140","0.140","0.350","0.350","0.350","0.350","0.350"]
["مطلوب مسافة فوق السقف المستعار >","mm","","","350","350","350","350","350","350","350"]
["Sound power level","التبريد","","dBA","63","63","57","57","61","66","66"]
["Dimensions","Unit","العرض","mm","700","700","1,000","1,000","1,400","1,400","1,400"]
["","","العمق","mm","700","700","700","700","700","700","700"]
["","","الارتفاع","mm","300","300","300","300","300","300","300"]
["الغلاف","اللون","","","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)"]
["الوزن","الوحدة","","kg","25","25","34","34","45","45","45"]
["Fan","External static pressure","عالٍ","باسكال","100","100","100","100","120","120","120"]
["","","الإسمي","باسكال","30","30","30","30","40","50","50"]
["ارتفاع الصرف","mm","","","625","625","625","625","625","625","625"]
["لوحة ديكور","الوزن","","kg","3.5","3.5","4.5","4.5","6.5","6.5","6.5"]
["","الطراز","","","BYBS45DJW1","BYBS45DJW1","BYBS71DJW1","BYBS71DJW1","BYBS125DJW1","BYBS125DJW1","BYBS125DJW1"]
["","الأبعاد","الارتفاع","mm","55","55","55","55","55","55","55"]
["","","العمق","mm","500","500","500","500","500","500","500"]
["","","العرض","mm","800","800","1,100","1,100","1,500","1,500","1,500"]
["","اللون","","","White (10Y9/0.5)","White (10Y9/0.5)","White (10Y9/0.5)","White (10Y9/0.5)","White (10Y9/0.5)","White (10Y9/0.5)","White (10Y9/0.5)"]
["Heating capacity","الاستطاعة الإجمالية","الإسمي","kW","4.0 (2)","5.5 (2)","7.0 (2)","8.0 (2)","11.2 (2)","14.0 (2)","15.5 (2)"]
["Power supply","الطور","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","الاسم","","","VE","VE","VE","VE","VE","VE","VE"]
["","Voltage","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","(1) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة‏، 19.0‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية الحوجلة الجافة؛ طول الأنابيب المكافئ: 7.5 م؛ الفرق في المستوى: 0 م","(1) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة‏، 19.0‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية الحوجلة الجافة؛ طول الأنابيب المكافئ: 7.5 م؛ الفرق في المستوى: 0 م","(1) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة‏، 19.0‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية الحوجلة الجافة؛ طول الأنابيب المكافئ: 7.5 م؛ الفرق في المستوى: 0 م","(1) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة‏، 19.0‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية الحوجلة الجافة؛ طول الأنابيب المكافئ: 7.5 م؛ الفرق في المستوى: 0 م","(1) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة‏، 19.0‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية الحوجلة الجافة؛ طول الأنابيب المكافئ: 7.5 م؛ الفرق في المستوى: 0 م","(1) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة‏، 19.0‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية الحوجلة الجافة؛ طول الأنابيب المكافئ: 7.5 م؛ الفرق في المستوى: 0 م","(1) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة‏، 19.0‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية الحوجلة الجافة؛ طول الأنابيب المكافئ: 7.5 م؛ الفرق في المستوى: 0 م"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["","","","","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat."]
["","","","","(4) - The sound pressure values are mentioned for a unit installed with rear suction.","(4) - The sound pressure values are mentioned for a unit installed with rear suction.","(4) - The sound pressure values are mentioned for a unit installed with rear suction.","(4) - The sound pressure values are mentioned for a unit installed with rear suction.","(4) - The sound pressure values are mentioned for a unit installed with rear suction.","(4) - The sound pressure values are mentioned for a unit installed with rear suction.","(4) - The sound pressure values are mentioned for a unit installed with rear suction."]
["","","","","(5) - فئة وحدة PED: Art3§3: مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC","(5) - فئة وحدة PED: Art3§3: مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC","(5) - فئة وحدة PED: Art3§3: مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC","(5) - فئة وحدة PED: Art3§3: مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC","(5) - فئة وحدة PED: Art3§3: مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC","(5) - فئة وحدة PED: Art3§3: مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC","(5) - فئة وحدة PED: Art3§3: مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC"]