{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":11,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQSG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQSG100L8Y1B","FCAG50AVEB / FCAG50AVEB / FCAG50AVEB / RZQSG125L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQSG100L8Y1B","FCAG60AVEB / FCAG60AVEB / RZQSG125L8Y1B","FCAG125AVEB / RZQSG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQSG140L7Y1B"]
["نطاق كفاءة استخدام الطاقة","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Cooling capacity","Nom.","","kW","","","","","","12.0 (1)","13.4 (1)"]
["تبريد المساحة","SEER","","","","","","","","5.30"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","","","","","793"]
["","الاستطاعة","Pdesign","kW","","","","","","12.0"]
["","فئة فعالية استهلاك الطاقة","","","","","","","","A"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","","","","","","8.03"]
["","SCOP/A","","","","","","","","4.01"]
["","فئة فعالية استهلاك الطاقة","","","","","","","","A+"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","","","","","2,804"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","","","","","","1,870"]
["","نسبة فعالية استهلاك الطاقة","","","","","","","","3.21 (3)","4.20 (3)"]
["","عامل الأداء","","","","","","","","3.41 (3)"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","","","","","A"]
["","","تدفئة","","","","","","","B"]
["Heating capacity","Nom.","","kW","","","","","","13.5 (2)","15.5 (2)"]
["Notes","","","","","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["","","","","","","","","","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]