{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":5,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXS-L3"]
[]
[]
[]
[]
["","","","","FCAG35BVEB / RXS35L3V1B"]
["Cooling capacity","Nom.","","kW","3.40"]
["Heating capacity","Nom.","","kW","4.20"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","455"]
["","عامل الأداء","","","3.50"]
["","نسبة فعالية استهلاك الطاقة","","","3.74"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A"]
["","","تدفئة","","B"]
["Piping connections","Drain","OD","mm","VP25 (القطر الخارجي 32؛ القطر الداخلي 25)"]
["","غاز","القطر الخارجي","mm","9.50"]
["","Liquid","القطر الخارجي","mm","6.35"]
["Notes","","","","(1) - عند التشغيل الطبيعي: +22°مئوية / + 32°مئوية"]
["","","","","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]
["","","","","(3) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","(4) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]