{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":13,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZQG100L8Y1B","FCAHG125GVEB / RZQG125L8Y1B","FCAHG100GVEB / RZQG71L8Y1B","FCAHG71GVEB / RZQG71L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG100L8Y1B","FCAHG140GVEB / RZQG100L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG140L7Y1B"]
["Cooling capacity","Nom.","","kW","","","","6.80 (1)","","","","","13.4 (1)"]
["تبريد المساحة","SEER","","","","","6.91","6.91","","","","","6.75"]
["","ηs,c","","%","","","","","","","","","266.9"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","","345","345","","","","","1,191"]
["","الاستطاعة","Pdesign","kW","","","6.80","6.80","","","","","13.4"]
["","فئة فعالية استهلاك الطاقة","","","","","A++","A++"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","","","7.60","7.60","","","","","11.8"]
["","SCOP/A","","","","","4.54","4.54","","","","","4.38"]
["","فئة فعالية استهلاك الطاقة","","","","","A+","A+"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","","2,344","2,344","","","","","3,766"]
["","ηs,h","","%","","","","","","","","","172.1"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","","","","830"]
["","نسبة فعالية استهلاك الطاقة","","","","","","4.09 (3)","","","","","3.18 (3)"]
["","عامل الأداء","","","","","","4.80 (3)","","","","","4.12 (3)"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","","","A"]
["","","تدفئة","","","","","A"]
["Heating capacity","Nom.","","kW","","","","7.50 (2)","","","","","15.5 (2)"]
["نطاق كفاءة استخدام الطاقة","","","","A+++ ~ D","A+++ ~ D","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Notes","","","","","","","(1) - التبريد: درجة الحرارة الداخلية 27 درجة مئوية للبويصلة الجافة، 19 درجة مئوية للبويصلة الرطبة؛ درجة الحرارة الخارجية 35 درجة مئوية للبويصلة الجافة؛ الطول المكافئ للمواسير: 7.5 متر؛ فرق المستوى: 0 متر","","","","","(1) - التبريد: درجة الحرارة الداخلية 27 درجة مئوية للبويصلة الجافة، 19 درجة مئوية للبويصلة الرطبة؛ درجة الحرارة الخارجية 35 درجة مئوية للبويصلة الجافة؛ الطول المكافئ للمواسير: 7.5 متر؛ فرق المستوى: 0 متر"]
["","","","","","","","(2) - التدفئة: درجة الحرارة الداخلية 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة؛ الطول المكافئ للمواسير: 7.5 متر ؛ فرق المستوى: 0 متر","","","","","(2) - التدفئة: درجة الحرارة الداخلية 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة؛ الطول المكافئ للمواسير: 7.5 متر ؛ فرق المستوى: 0 متر"]
["","","","","","","","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","","","","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["Outdoor unit","","","","","","","","RZQG100L8Y1","RZQG100L8Y1","RZQG125L8Y1","RZQG125L8Y1"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","","","","","A","A++","A","A++"]
["","الاستطاعة","Pdesign","kW","","","","","9.50","9.50","12.0","12.0"]
["","SEER","","","","","","","5.10","7.00","5.10","6.61"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","","","","652","475","824","636"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","","","","","A","A++","A","A++"]
["","الاستطاعة","Pdesign","kW","","","","","11.30","11.30","12.71","12.66"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","","","","","3.80","4.80","3.80","4.63"]
["","Pdh استطاعة التدفئة عند -10°","","kW","","","","","9.66","9.69","11.4","11.5"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","","","","4164","3296","4683","3829"]