{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":11,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQ-C8"]
[]
[]
[]
[]
["","","","","FCQ35C8VEB","FCQ50C8VEB","FCQ60C8VEB","FCQ71C8VEB","FCQ100C8VEB","FCQ125C8VEB","FCQ140C8VEB"]
["Sound pressure level","Heating","High","dBA","31","31","33","34","37","41","42"]
["","","Low","dBA","27","27","28","28","32","35","35"]
["","Cooling","Low","dBA","27","27","28","28","32","35","35"]
["","","High","dBA","31","31","33","33","37","41","41"]
["Standard Accessories","Operation manual","","","Operation manual","Operation manual","Operation manual","Operation manual","Operation manual","Operation manual","Operation manual"]
["","Installation manual","","","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual"]
["","خرطوم الصرف","","","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف"]
["","مشبك لخرطوم الصرف","","","مشبك لخرطوم الصرف","مشبك لخرطوم الصرف","مشبك لخرطوم الصرف","مشبك لخرطوم الصرف","مشبك لخرطوم الصرف","مشبك لخرطوم الصرف","مشبك لخرطوم الصرف"]
["","حلقة للدعامة الحاملة","","","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة"]
["","مسامير لولبية","","","مسامير لولبية","مسامير لولبية","مسامير لولبية","مسامير لولبية","مسامير لولبية","مسامير لولبية","مسامير لولبية"]
["","دليل التركيب","","","دليل التركيب","دليل التركيب","دليل التركيب","دليل التركيب","دليل التركيب","دليل التركيب","دليل التركيب"]
["","عازل لأدوات التثبيت","","","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت"]
["","لباد مانع للتسريب","","","لباد مانع للتسريب","لباد مانع للتسريب","لباد مانع للتسريب","لباد مانع للتسريب","لباد مانع للتسريب","لباد مانع للتسريب","لباد مانع للتسريب"]
["","لبادة مانعة التسريب للمصرف","","","لبادة مانعة التسريب للمصرف","لبادة مانعة التسريب للمصرف","لبادة مانعة التسريب للمصرف","لبادة مانعة التسريب للمصرف","لبادة مانعة التسريب للمصرف","لبادة مانعة التسريب للمصرف","لبادة مانعة التسريب للمصرف"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","غاز","القطر الخارجي","mm","9.52","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Drain","","","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)"]
["Sound power level","التبريد","","dBA","49","49","51","51","54","58","58"]
["Dimensions","Unit","العرض","mm","840","840","840","840","840","840","840"]
["","","العمق","mm","840","840","840","840","840","840","840"]
["","","الارتفاع","mm","204","204","204","204","246","246","246"]
["الغلاف","المادة","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["الوزن","الوحدة","","kg","19","19","19","21","23","23","23"]
["لوحة ديكور","الوزن","","kg","5.5","5.5","5.5","5.5","5.5","5.5","5.5"]
["","الطراز","","","BYCQ140CW1","BYCQ140CW1","BYCQ140CW1","BYCQ140CW1","BYCQ140CW1","BYCQ140CW1","BYCQ140CW1"]
["","الأبعاد","الارتفاع","mm","50","50","50","50","50","50","50"]
["","","العمق","mm","950","950","950","950","950","950","950"]
["","","العرض","mm","950","950","950","950","950","950","950"]
["","اللون","","","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)"]
["Power supply","الطور","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","الاسم","","","VE","VE","VE","VE","VE","VE","VE"]
["","Voltage","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","(1) - The sound pressure values are mentioned for a unit installed with rear suction.","(1) - The sound pressure values are mentioned for a unit installed with rear suction.","(1) - The sound pressure values are mentioned for a unit installed with rear suction.","(1) - The sound pressure values are mentioned for a unit installed with rear suction.","(1) - The sound pressure values are mentioned for a unit installed with rear suction.","(1) - The sound pressure values are mentioned for a unit installed with rear suction.","(1) - The sound pressure values are mentioned for a unit installed with rear suction."]
["","","","","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates."]
["","","","","(3) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt."]
["","","","","(4) - Maximum allowable voltage range variation between phases is 2%.","(4) - Maximum allowable voltage range variation between phases is 2%.","(4) - Maximum allowable voltage range variation between phases is 2%.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","(5) - Select wire size based on the value of MCA","(5) - Select wire size based on the value of MCA","(5) - Select wire size based on the value of MCA","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","(6) - Instead of a fuse, use a circuit breaker","(6) - Instead of a fuse, use a circuit breaker","(6) - Instead of a fuse, use a circuit breaker","(6) - Select wire size based on the larger value of MCA or TOCA","(6) - Select wire size based on the larger value of MCA or TOCA","(6) - Select wire size based on the larger value of MCA or TOCA","(6) - Select wire size based on the larger value of MCA or TOCA"]
["","","","","","","","(7) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(7) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(7) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(7) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker)."]