{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":8,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-E"]
[]
[]
[]
[]
["","","","","FCQG71EVEB","FCQG100EVEB","FCQG125EVEB","FCQG140EVEB"]
["Sound pressure level","Heating","High","dBA","36","44","45","45"]
["","","Nom.","dBA","33","39","41","41"]
["","","Low","dBA","29","33","35","37"]
["","Cooling","Low","dBA","29","33","35","37"]
["","","High","dBA","36","44","45","45"]
["","","Nom.","dBA","33","39","41","41"]
["Piping connections","Liquid","القطر الخارجي","mm","9.52","9.52","9.52","9.52"]
["","غاز","القطر الخارجي","mm","15.9","15.9","15.9","15.9"]
["","Drain","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Sound power level","التبريد","","dBA","53","61","61","61"]
["Dimensions","Unit","العرض","mm","840","840","840","840"]
["","","العمق","mm","840","840","840","840"]
["","","الارتفاع","mm","288","288","288","288"]
["الغلاف","المادة","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["الوزن","الوحدة","","kg","25","25","25","25"]
["Power supply","الطور","","","1~","1~","1~","1~"]
["","Frequency","","Hz","50","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240","220-240"]